<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>Key</text>
<text>Tx</text>
<text>Piezo</text>
<text>On</text>
<text>Ext. Spkr.</text>
<wire x1="25.0444" y1="50.8" x2="81.6864" y2="50.8" width="0.4064" layer="20"/>
<wire x1="81.6864" y1="50.8" x2="81.6864" y2="7.62" width="0.4064" layer="20"/>
<wire x1="81.6864" y1="7.62" x2="25.0444" y2="7.62" width="0.4064" layer="20"/>
<wire x1="25.0444" y1="7.62" x2="25.0444" y2="50.8" width="0.4064" layer="20"/>
<hole x="30.1244" y="19.304" drill="3.2"/>
<hole x="78.6384" y="47.752" drill="3.2"/>
<hole x="38.7604" y="48.006" drill="3.2"/>
<hole x="78.8924" y="10.414" drill="3.2"/>
<text>CR2032</text>
<text>Msg 1</text>
<text>Msg 2</text>
<text>Cmd.</text>
<text>www.electroresales.com</text>
<text>Tip</text>
<text>Ring</text>
<text>Dah</text>
<text>Dit</text>
<text>Dit</text>
<text>Dah</text>
<text>Version F17</text>
<text>Tip</text>
<text>Ring</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT54E">
<description>&lt;b&gt;SOT-54&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH-SIDEEZ">
</package>
<package name="BATTCOM_20MM_PTH">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AL60P">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16F628A" library="SparkFun-DigitalIC" package="DIL18" value="PIC16F628-DIP">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT54E" value="BS170">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="S4" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="SWITCH-MOMENTARY-2SIDE_EZ"/>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="SWITCH-MOMENTARY-2SIDE_EZ"/>
<element name="S6" library="SparkFun-Electromechanical" package="TACTILE-PTH-SIDEEZ" value="SWITCH-MOMENTARY-2SIDE_EZ"/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCOM_20MM_PTH" value="">
<attribute name="VALUE"/>
</element>
<element name="SP1" library="adafruit" package="AL60P" value="SPEAKER/AL60P">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="16F628A" pad="16"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="3"/>
<contactref element="SP1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="SLEEVE"/>
<contactref element="Q1" pad="S"/>
<contactref element="16F628A" pad="5"/>
<contactref element="JP2" pad="SLEEVE"/>
<contactref element="JP6" pad="1"/>
<contactref element="S4" pad="2"/>
<contactref element="S5" pad="2"/>
<contactref element="S6" pad="2"/>
<contactref element="BAT1" pad="2"/>
<contactref element="SP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="D"/>
<contactref element="JP1" pad="TIP"/>
<contactref element="JP1" pad="RING"/>
</signal>
<signal name="N$6">
<contactref element="16F628A" pad="15"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="VCC">
<contactref element="16F628A" pad="14"/>
<contactref element="BAT1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="16F628A" pad="11"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="16F628A" pad="10"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JP4" pad="3"/>
<contactref element="JP2" pad="RING"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP4" pad="1"/>
<contactref element="JP2" pad="TIP"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="S4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="A"/>
<contactref element="16F628A" pad="13"/>
<contactref element="S6" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="16F628A" pad="12"/>
<contactref element="D2" pad="A"/>
<contactref element="S5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
