<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<circle x="2" y="78" radius="1.3" width="0.254" layer="20"/>
<circle x="98" y="78" radius="1.3" width="0.254" layer="20"/>
<circle x="98" y="2" radius="1.3" width="0.254" layer="20"/>
<text>Red de Acción Comunitaria
reaccion.net
CODENAME Torogoz
BATCH 0002 | 09/11/2015
Designed in El Salvador
</text>
<circle x="2" y="2" radius="1.3" width="0.254" layer="20"/>
<text>L4</text>
<text>USER_INTERFACE</text>
<text>DISPLAY_SDCARD_CONN</text>
<text>SIMCARD_CONN</text>
<text>IC_11</text>
<text>USER_GPIO</text>
<text>IC_16</text>
</plain>
<libraries>
<library name="custom_componentsv0.9">
<description>The LM2621 is a high efficiency, step-up DC-DC switching regulator for battery-powered and low input
voltage systems.</description>
<packages>
<package name="SOT23-5">
</package>
<package name="1210-POLARIZED">
</package>
<package name="1206-POL">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="custom_components">
<packages>
<package name="SOT95P300X145-5N">
</package>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="custom-components">
<packages>
<package name="M10478">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="SO14">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="SOT665">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="U.FL">
</package>
<package name="SIMHOLDER3">
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="1X10">
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="sim900">
<packages>
<package name="SIM900">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Bluetooth HC-05">
<description>Bluetooth HC05 Module. See http://mcuoneclipse.com/2013/02/14/bluetooth-with-the-freedom-board/</description>
<packages>
<package name="BLUETOOTH_SMD">
<description>HC-05</description>
</package>
</packages>
</library>
<library name="maxstream">
<description>&lt;b&gt;MaxSream&lt;/b&gt; XBee Products&lt;p&gt;
http://www.maxstream.net</description>
<packages>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
</packages>
</library>
<library name="Teensy3.0">
<packages>
<package name="TEENSY_3.0_ALLPINS">
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QSOP24">
<description>&lt;b&gt;QSOP 24&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7313.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
<library name="Reaccion-Custom">
<packages>
<package name="MS5637-02BA03">
</package>
<package name="2X2-DFN">
</package>
</packages>
</library>
<library name="inductor-bourns">
<description>&lt;b&gt;Bourns Inductors  - v1.01, 03/01/2010&lt;/b&gt;&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SRR4028">
<description>&lt;B&gt;POWER INDUCTOR&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC_6" library="custom_components" package="SOT95P300X145-5N" value="MCP73831T-2ATI/OT">
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="OC_NEWARK" value="84R5196"/>
<attribute name="MPN" value="MCP73831T-2ATI/OT"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1834890"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="2K">
<attribute name="NAME"/>
</element>
<element name="IC_1" library="custom_components" package="SOT23-6L" value="LTC4412">
<attribute name="NAME"/>
</element>
<element name="D4" library="custom_components" package="SOD123" value="1N5819HW-7-F">
<attribute name="NAME"/>
</element>
<element name="Q9" library="custom_components" package="SOT23" value="SI2301CDS">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="IC_3" library="adafruit" package="SOT23-5L" value="LP298XS">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="470pF">
<attribute name="NAME"/>
</element>
<element name="IC_16" library="custom-components" package="M10478" value="M10478"/>
<element name="IC_19" library="custom-components" package="SO08" value="SST25WF040B">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="U.FL" value="U.FL"/>
<element name="L1" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="0805" value="2.2uF">
<attribute name="NAME"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="C19" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="IC_17" library="custom-components" package="SO14" value="TXB0104">
<attribute name="NAME"/>
</element>
<element name="IC_18" library="custom-components" package="SO14" value="TXB0104">
<attribute name="NAME"/>
</element>
<element name="IC_9" library="sim900" package="SIM900" value="SIM900">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
</element>
<element name="T2" library="transistor" package="SOT23" value="BC847">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="IC_11" library="custom-components" package="SOT665" value="SMF05C"/>
<element name="SIMCONN" library="SparkFun-Connectors" package="SIMHOLDER3" value="SIMHOLDER3"/>
<element name="C20" library="SparkFun-Capacitors" package="0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C21" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
</element>
<element name="IC_10" library="custom-components" package="SO14" value="TXB0104">
<attribute name="NAME"/>
</element>
<element name="J$1" library="SparkFun-Connectors" package="SMA-EDGE" value="SMA_EDGE"/>
<element name="R19" library="SparkFun-Resistors" package="0805" value="0">
<attribute name="NAME"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="0">
<attribute name="NAME"/>
</element>
<element name="C22" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC_15" library="Bluetooth HC-05" package="BLUETOOTH_SMD" value="HC_05">
<attribute name="NAME"/>
</element>
<element name="Q1" library="adafruit" package="SOT23" value="2N7002K-T1-E3">
<attribute name="NAME"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="XB1" library="maxstream" package="XBEE-PRO" value="XBEE-PRO">
<attribute name="OC_NEWARK" value="42M2667"/>
<attribute name="MPN" value="XBP24-AWI-001"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1337916"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
</element>
<element name="IC_12" library="Teensy3.0" package="TEENSY_3.0_ALLPINS" value="TEENSY_3.0_ALLPINS">
<attribute name="NAME"/>
</element>
<element name="IC_13" library="maxim" package="QSOP24" value="MAX7313AEG">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="53K7268"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="MAX7313AEG+"/>
<attribute name="NAME"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="SJ2" library="SparkFun-Retired" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="SJ3" library="SparkFun-Retired" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead" package="2X05" value="UI">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="BATT">
<attribute name="NAME"/>
</element>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM" value="3.7V">
<attribute name="PROD_ID" value="BATT-08044"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD-REDUNDANT">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
</element>
<element name="R42" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R43" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R44" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R45" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R46" library="SparkFun-Resistors" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="Q3" library="adafruit" package="SOT23" value="2N7002K-T1-E3">
<attribute name="NAME"/>
</element>
<element name="R47" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R49" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="BUZZER" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="BATT">
<attribute name="NAME"/>
</element>
<element name="IC_8" library="Reaccion-Custom" package="MS5637-02BA03" value="MS5637-02BA03">
<attribute name="NAME"/>
</element>
<element name="IC_7" library="Reaccion-Custom" package="2X2-DFN" value="MMA8653FC">
<attribute name="NAME"/>
</element>
<element name="C24" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C25" library="SparkFun-Capacitors" package="0805" value="1uF"/>
<element name="C27" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C28" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="custom_componentsv0.9" package="SOT23-5" value="LT1935ES5">
<attribute name="NAME"/>
</element>
<element name="L6" library="inductor-bourns" package="SRR4028" value="1.8uH">
<attribute name="NAME"/>
</element>
<element name="CIN" library="custom_componentsv0.9" package="1210-POLARIZED" value="100uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="68pF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="47uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K"/>
<element name="R13" library="SparkFun-Resistors" package="0805" value="30K">
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="DOUT" library="custom_componentsv0.9" package="1206-POL" value="SD1206S040S2R0">
<attribute name="NAME"/>
</element>
<element name="U$2" library="custom_componentsv0.9" package="SOT23-5" value="LT1935ES5">
<attribute name="NAME"/>
</element>
<element name="L3" library="inductor-bourns" package="SRR4028" value="1.8uH">
<attribute name="NAME"/>
</element>
<element name="CIN1" library="custom_componentsv0.9" package="1210-POLARIZED" value="100uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.22uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="68pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="84.5K">
<attribute name="NAME"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="DOUT1" library="custom_componentsv0.9" package="1206-POL" value="SD1206S040S2R0">
<attribute name="NAME"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="USB-B-PTH" value="USB-B">
<attribute name="PROD_ID" value="CONN-08278"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="MIC5219 3.3V">
<attribute name="PROD_ID" value="VREG-09872"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="470pF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="IC_6" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="IC_1" pad="2"/>
<contactref element="IC_1" pad="2"/>
<contactref element="IC_1" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="IC_3" pad="2"/>
<contactref element="IC_16" pad="28"/>
<contactref element="IC_16" pad="27"/>
<contactref element="IC_16" pad="25"/>
<contactref element="IC_16" pad="24"/>
<contactref element="IC_16" pad="19"/>
<contactref element="IC_16" pad="1"/>
<contactref element="IC_16" pad="2"/>
<contactref element="IC_16" pad="3"/>
<contactref element="IC_16" pad="5"/>
<contactref element="IC_16" pad="7"/>
<contactref element="IC_16" pad="9"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="IC_19" pad="4"/>
<contactref element="C19" pad="1"/>
<contactref element="IC_16" pad="15"/>
<contactref element="IC_17" pad="7"/>
<contactref element="IC_17" pad="7"/>
<contactref element="IC_18" pad="7"/>
<contactref element="IC_9" pad="17"/>
<contactref element="IC_9" pad="18"/>
<contactref element="IC_9" pad="29"/>
<contactref element="IC_9" pad="39"/>
<contactref element="IC_9" pad="45"/>
<contactref element="IC_9" pad="46"/>
<contactref element="IC_9" pad="53"/>
<contactref element="IC_9" pad="54"/>
<contactref element="IC_9" pad="58"/>
<contactref element="IC_9" pad="59"/>
<contactref element="IC_9" pad="61"/>
<contactref element="IC_9" pad="62"/>
<contactref element="IC_9" pad="63"/>
<contactref element="IC_9" pad="64"/>
<contactref element="IC_9" pad="65"/>
<contactref element="R12" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="SIMCONN" pad="6"/>
<contactref element="IC_11" pad="2"/>
<contactref element="IC_10" pad="7"/>
<contactref element="IC_10" pad="7"/>
<contactref element="J$1" pad="GND@0"/>
<contactref element="J$1" pad="GND@3"/>
<contactref element="J$1" pad="GND@2"/>
<contactref element="J$1" pad="GND@1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="XB1" pad="10"/>
<contactref element="XB1" pad="14"/>
<contactref element="JP1" pad="10"/>
<contactref element="IC_13" pad="12"/>
<contactref element="JP2" pad="10"/>
<contactref element="JP3" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="IC_12" pad="AGND"/>
<contactref element="IC_12" pad="GND"/>
<contactref element="IC_12" pad="GND2"/>
<contactref element="IC_12" pad="GND1"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="R44" pad="1"/>
<contactref element="J1" pad="P$1"/>
<contactref element="L2" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="R47" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="IC_7" pad="8"/>
<contactref element="IC_7" pad="7"/>
<contactref element="IC_7" pad="6"/>
<contactref element="IC_8" pad="4"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="CIN" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="CIN1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="JP6" pad="GND"/>
<contactref element="C11" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="D4" pad="1"/>
<contactref element="Q9" pad="2"/>
<contactref element="IC_1" pad="6"/>
<contactref element="CIN" pad="1"/>
<contactref element="L6" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="CIN1" pad="1"/>
<contactref element="U$2" pad="5"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="XB1" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="IC_7" pad="1"/>
<contactref element="IC_7" pad="9"/>
<contactref element="IC_8" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="IC_15" pad="12"/>
<contactref element="C24" pad="2"/>
<contactref element="R46" pad="1"/>
<contactref element="R45" pad="1"/>
<contactref element="IC_13" pad="24"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="IC_12" pad="AREF"/>
</signal>
<signal name="5V">
<contactref element="IC_12" pad="VIN"/>
<contactref element="DOUT" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC_3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="IC_17" pad="14"/>
<contactref element="IC_18" pad="14"/>
<contactref element="R3" pad="2"/>
<contactref element="IC_10" pad="14"/>
<contactref element="JP1" pad="9"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="IC_18" pad="8"/>
<contactref element="IC_17" pad="8"/>
<contactref element="IC_3" pad="3"/>
<contactref element="IC_10" pad="8"/>
</signal>
<signal name="VEXT">
<contactref element="D4" pad="2"/>
<contactref element="IC_6" pad="4"/>
<contactref element="C7" pad="2"/>
<contactref element="JP6" pad="VBUS"/>
</signal>
<signal name="CHG_STAT">
<contactref element="R3" pad="1"/>
<contactref element="IC_6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R4" pad="2"/>
<contactref element="IC_6" pad="5"/>
</signal>
<signal name="VBATT">
<contactref element="C8" pad="2"/>
<contactref element="IC_6" pad="3"/>
<contactref element="IC_1" pad="1"/>
<contactref element="Q9" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="IC_9" pad="55"/>
<contactref element="IC_9" pad="56"/>
<contactref element="IC_9" pad="57"/>
</signal>
<signal name="N$12">
<contactref element="IC_1" pad="5"/>
<contactref element="Q9" pad="1"/>
</signal>
<signal name="PWR_STAT">
<contactref element="IC_1" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC_3" pad="4"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="1V8">
<contactref element="IC_3" pad="5"/>
<contactref element="C9" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="IC_16" pad="8"/>
<contactref element="R6" pad="1"/>
<contactref element="IC_19" pad="7"/>
<contactref element="IC_19" pad="8"/>
<contactref element="R8" pad="1"/>
<contactref element="IC_19" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="IC_17" pad="1"/>
<contactref element="IC_18" pad="1"/>
</signal>
<signal name="12V">
<contactref element="BUZZER" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="DOUT1" pad="2"/>
</signal>
<signal name="12V_EN">
<contactref element="IC_13" pad="17"/>
<contactref element="R1" pad="1"/>
<contactref element="IC_12" pad="26"/>
</signal>
<signal name="N$15">
<contactref element="IC_16" pad="6"/>
<contactref element="L2" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="L1" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="J1" pad="P$3"/>
<contactref element="IC_16" pad="4"/>
</signal>
<signal name="GPS_RX_1V8">
<contactref element="IC_16" pad="21"/>
<contactref element="C18" pad="2"/>
<contactref element="IC_17" pad="2"/>
</signal>
<signal name="GPS_TX_1V8">
<contactref element="IC_16" pad="20"/>
<contactref element="C17" pad="2"/>
<contactref element="IC_17" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="IC_16" pad="23"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="GPS_ONOFF_1V8">
<contactref element="IC_16" pad="26"/>
<contactref element="IC_17" pad="4"/>
</signal>
<signal name="GPS_TM_1V8">
<contactref element="IC_16" pad="11"/>
<contactref element="IC_17" pad="5"/>
</signal>
<signal name="GPS_RST_1V8">
<contactref element="IC_16" pad="10"/>
<contactref element="IC_18" pad="5"/>
</signal>
<signal name="GPS_WU_1V8">
<contactref element="IC_16" pad="18"/>
<contactref element="IC_18" pad="4"/>
</signal>
<signal name="GPS_SPI_CLK">
<contactref element="IC_19" pad="6"/>
<contactref element="R8" pad="2"/>
<contactref element="IC_16" pad="14"/>
</signal>
<signal name="GPS_SPI_MOSI">
<contactref element="IC_19" pad="5"/>
<contactref element="IC_16" pad="12"/>
</signal>
<signal name="GPS_SPI_CS">
<contactref element="IC_19" pad="1"/>
<contactref element="IC_16" pad="16"/>
</signal>
<signal name="GPS_SPI_MISO">
<contactref element="IC_19" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="IC_16" pad="13"/>
</signal>
<signal name="GPS_RX">
<contactref element="IC_17" pad="13"/>
<contactref element="IC_12" pad="8"/>
</signal>
<signal name="GPS_TX">
<contactref element="IC_17" pad="12"/>
<contactref element="IC_12" pad="7"/>
</signal>
<signal name="GPS_ONOFF">
<contactref element="IC_17" pad="11"/>
<contactref element="IC_12" pad="14/A0"/>
</signal>
<signal name="GPS_TM">
<contactref element="IC_17" pad="10"/>
<contactref element="IC_12" pad="15/A1"/>
</signal>
<signal name="GPS_WU">
<contactref element="IC_18" pad="11"/>
<contactref element="IC_12" pad="16/A2"/>
</signal>
<signal name="GPS_RST">
<contactref element="IC_18" pad="10"/>
<contactref element="IC_12" pad="17/A3"/>
</signal>
<signal name="PWRKEY">
<contactref element="IC_9" pad="1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="SIM900_RI_2V8">
<contactref element="IC_9" pad="4"/>
<contactref element="IC_10" pad="5"/>
</signal>
<signal name="SIM900_TX_2V8">
<contactref element="IC_9" pad="9"/>
<contactref element="IC_10" pad="3"/>
</signal>
<signal name="SIM900_RX_2V8">
<contactref element="IC_9" pad="10"/>
<contactref element="IC_10" pad="2"/>
</signal>
<signal name="2V8">
<contactref element="IC_9" pad="15"/>
<contactref element="IC_10" pad="1"/>
</signal>
<signal name="NRESET">
<contactref element="IC_9" pad="16"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="RF_ANT">
<contactref element="IC_9" pad="60"/>
<contactref element="R20" pad="1"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="SIM900_STATUS_2V8">
<contactref element="IC_9" pad="66"/>
<contactref element="IC_10" pad="4"/>
</signal>
<signal name="SIM_VDD">
<contactref element="IC_9" pad="30"/>
<contactref element="SIMCONN" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="IC_11" pad="1"/>
</signal>
<signal name="SIM_RST">
<contactref element="IC_9" pad="33"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="T1" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="T2" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="SIM900_RESET">
<contactref element="R11" pad="1"/>
<contactref element="IC_12" pad="21/A7"/>
</signal>
<signal name="SIM900_PWR">
<contactref element="R9" pad="1"/>
<contactref element="IC_12" pad="2"/>
</signal>
<signal name="SIM_CLK">
<contactref element="R17" pad="1"/>
<contactref element="IC_9" pad="32"/>
</signal>
<signal name="N$29">
<contactref element="R16" pad="2"/>
<contactref element="IC_11" pad="6"/>
<contactref element="SIMCONN" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="SIMCONN" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="IC_11" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="SIMCONN" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="IC_11" pad="3"/>
</signal>
<signal name="SIM900_RX">
<contactref element="IC_10" pad="13"/>
<contactref element="IC_12" pad="10"/>
</signal>
<signal name="SIM900_TX">
<contactref element="IC_10" pad="12"/>
<contactref element="IC_12" pad="9"/>
</signal>
<signal name="SIM900_STATUS">
<contactref element="IC_10" pad="11"/>
<contactref element="IC_12" pad="31"/>
</signal>
<signal name="SIM900_RI">
<contactref element="IC_10" pad="10"/>
<contactref element="IC_12" pad="30"/>
</signal>
<signal name="N$28">
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="R19" pad="2"/>
<contactref element="J$1" pad="SIG"/>
</signal>
<signal name="BT_TX">
<contactref element="IC_15" pad="1"/>
<contactref element="IC_12" pad="24"/>
</signal>
<signal name="BT_RX">
<contactref element="IC_15" pad="2"/>
<contactref element="IC_12" pad="25"/>
</signal>
<signal name="BT_CMD">
<contactref element="IC_15" pad="34"/>
<contactref element="IC_15" pad="26"/>
<contactref element="IC_12" pad="33"/>
</signal>
<signal name="N$25">
<contactref element="IC_15" pad="13"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC_15" pad="21"/>
<contactref element="IC_15" pad="22"/>
</signal>
<signal name="N$34">
<contactref element="R22" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="BT_EN">
<contactref element="R23" pad="2"/>
<contactref element="IC_12" pad="27"/>
</signal>
<signal name="XBEE_RESET">
<contactref element="XB1" pad="5"/>
<contactref element="IC_12" pad="28"/>
</signal>
<signal name="XBEE_SLEEP">
<contactref element="XB1" pad="13"/>
<contactref element="IC_12" pad="22/A8"/>
</signal>
<signal name="XBEE_TX">
<contactref element="XB1" pad="2"/>
<contactref element="IC_12" pad="0"/>
</signal>
<signal name="XBEE_RX">
<contactref element="XB1" pad="3"/>
<contactref element="IC_12" pad="1"/>
</signal>
<signal name="DISPLAY_BL">
<contactref element="JP1" pad="1"/>
<contactref element="IC_12" pad="20/A6"/>
</signal>
<signal name="SPI1_SCK">
<contactref element="JP1" pad="2"/>
<contactref element="IC_12" pad="13"/>
</signal>
<signal name="SPI1_MISO">
<contactref element="JP1" pad="3"/>
<contactref element="IC_12" pad="11"/>
</signal>
<signal name="SPI1_MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="IC_12" pad="12"/>
</signal>
<signal name="SPI1_CS">
<contactref element="JP1" pad="5"/>
<contactref element="IC_12" pad="6"/>
</signal>
<signal name="DISPLAY_SDCS">
<contactref element="JP1" pad="6"/>
<contactref element="IC_12" pad="5"/>
</signal>
<signal name="SPI1_RST">
<contactref element="JP1" pad="7"/>
<contactref element="IC_12" pad="3"/>
</signal>
<signal name="DISPLAY_DC">
<contactref element="JP1" pad="8"/>
<contactref element="IC_12" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="IC_12" pad="3.3V"/>
<contactref element="IC_12" pad="3.3V1"/>
<contactref element="IC_12" pad="3.3V2"/>
</signal>
<signal name="SCL">
<contactref element="IC_12" pad="19/A5"/>
<contactref element="IC_13" pad="22"/>
<contactref element="R46" pad="2"/>
<contactref element="IC_7" pad="2"/>
<contactref element="IC_8" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC_12" pad="18/A4"/>
<contactref element="IC_13" pad="23"/>
<contactref element="R45" pad="2"/>
<contactref element="IC_7" pad="10"/>
<contactref element="IC_8" pad="2"/>
</signal>
<signal name="ANALOG_XAXIS">
<contactref element="JP2" pad="6"/>
<contactref element="IC_12" pad="A13"/>
</signal>
<signal name="ANALOG_YAXIS">
<contactref element="JP2" pad="8"/>
<contactref element="IC_12" pad="A12"/>
</signal>
<signal name="BTN_A">
<contactref element="IC_13" pad="10"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="BTN_B">
<contactref element="IC_13" pad="11"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="BTN_C">
<contactref element="IC_13" pad="13"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="BTN_D">
<contactref element="IC_13" pad="14"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="BTN_E">
<contactref element="JP2" pad="2"/>
<contactref element="IC_13" pad="15"/>
</signal>
<signal name="BTN_F">
<contactref element="JP2" pad="4"/>
<contactref element="IC_13" pad="16"/>
</signal>
<signal name="IO_INT0">
<contactref element="IC_13" pad="1"/>
<contactref element="IC_12" pad="32"/>
</signal>
<signal name="N$37">
<contactref element="IC_13" pad="21"/>
<contactref element="SJ1" pad="2"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC_13" pad="3"/>
<contactref element="R28" pad="1"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="IC_13" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="IC_12" pad="VBAT"/>
<contactref element="BAT1" pad="PWR@1"/>
</signal>
<signal name="VUSB">
<contactref element="IC_12" pad="VUSB"/>
</signal>
<signal name="RESET">
<contactref element="IC_12" pad="RESET"/>
<contactref element="R42" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="R43" pad="1"/>
<contactref element="IC_12" pad="A10"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="BUZZER_ACT">
<contactref element="IC_12" pad="23/A9"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="Q3" pad="1"/>
<contactref element="R49" pad="1"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="BUZZER" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="SIM_DATA">
<contactref element="IC_9" pad="31"/>
<contactref element="R18" pad="2"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="1"/>
<contactref element="L6" pad="2"/>
<contactref element="DOUT" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="R13" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="R14" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="DOUT1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R15" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="R21" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="4"/>
<contactref element="C11" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
