<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<text>goodman_jason@wheatonma.edu
Thermistor Feather Board 1.0
</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-6">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -6 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FEATHERWING">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MS1" library="adafruit" package="FEATHERWING" value="FEATHERWING"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08375"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="THERM1">
<contactref element="MS1" pad="5"/>
<contactref element="R1" pad="P$2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="THERM2">
<contactref element="R2" pad="P$2"/>
<contactref element="MS1" pad="6"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="THERM3">
<contactref element="R3" pad="P$2"/>
<contactref element="MS1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="THERM4">
<contactref element="R4" pad="P$2"/>
<contactref element="MS1" pad="8"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="THERM5">
<contactref element="R5" pad="P$2"/>
<contactref element="MS1" pad="9"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="R5" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="MS1" pad="4"/>
</signal>
<signal name="3V">
<contactref element="MS1" pad="2"/>
<contactref element="MS1" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
