<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<hole x="2.5" y="2.5" drill="3.2"/>
<hole x="2.5" y="47.5" drill="3.2"/>
<hole x="47.5" y="2.5" drill="3.2"/>
<hole x="47.5" y="47.5" drill="3.2"/>
<wire x1="1.5" y1="50" x2="48.5" y2="50" width="0" layer="20"/>
<wire x1="50" y1="1.5" x2="50" y2="48.5" width="0" layer="20"/>
<wire x1="1.5" y1="0" x2="48.5" y2="0" width="0" layer="20"/>
<wire x1="0" y1="48.5" x2="0" y2="1.5" width="0" layer="20"/>
<wire x1="1.5" y1="50" x2="0" y2="48.5" width="0" layer="20" curve="90"/>
<wire x1="50" y1="48.5" x2="48.5" y2="50" width="0" layer="20" curve="90"/>
<wire x1="48.5" y1="0" x2="50" y2="1.5" width="0" layer="20" curve="90"/>
<wire x1="0" y1="1.5" x2="1.5" y2="0" width="0" layer="20" curve="90"/>
<text>STorM32 BGC</text>
<text>STorM32 BGC v1.3</text>
<text>by Martinez &amp; OlliW</text>
<text>Layout and Design</text>
<text>I2C</text>
<text>I2C</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>3.3V</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>MOT0</text>
<text>MOT1</text>
<text>MOT2</text>
<text>MOT0</text>
<text>MOT1</text>
<text>MOT2</text>
<text>SWD</text>
<text>AUX</text>
<text>UART</text>
<text>POT</text>
<text>BUT</text>
<text>RC</text>
<text>RC2</text>
<text>GND</text>
<text>0</text>
<text>3</text>
<text>RC</text>
<text>RC2</text>
<text>3.3V</text>
<text>SWCLK</text>
<text>SWDIO</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>GND</text>
<text>Tx</text>
<text>Rx</text>
<text>GND</text>
<text>UART</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3.3V</text>
<text>GND</text>
<text>RESET</text>
<text>BOOT0</text>
<text>Bluetooth HC06</text>
<text>GND</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3.3V</text>
<text>BUT</text>
<text>POT</text>
<text>Layout and Design</text>
<text>by Martinez and OlliW</text>
<text>BT</text>
<text>LED1</text>
<text>LED0</text>
<text>www.olliw.eu</text>
<text>www.olliw.eu</text>
<text>! 3.3V max 3.3V max !</text>
<text>18V</text>
<text>This is open source under
the terms of the TAPR
Open Hardware License
http://www.tapr.org/ohl.html</text>
<text>SWD</text>
<text>GND</text>
<text>3.3V</text>
<text>I2C#2</text>
<text>IR</text>
<text>GND</text>
<text>IR</text>
<text>GND</text>
<text>3.3V</text>
<text>SCL</text>
<text>SDA</text>
<text>IR</text>
<text>Rx</text>
<text>Tx</text>
<text>SPK</text>
<text>Spk</text>
<text>SB</text>
<text>v1.3</text>
</plain>
<libraries>
<library name="# SparkFun">
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="# stdlib">
<packages>
<package name="CRYTSAL-SMD-5X3">
</package>
<package name="DFN8">
</package>
<package name="SO08">
</package>
<package name="1X1_WITHOUT">
</package>
<package name="MOLEX-53261-04-SMD-FLAT">
</package>
<package name="SOD123W-DIODE">
</package>
</packages>
</library>
<library name="# SparkFun2">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DPAK">
</package>
<package name="QFN-24">
</package>
<package name="1X03">
</package>
<package name="1X05">
</package>
<package name="1X02">
</package>
<package name="1X04">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="# dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SW_TACT_3X6">
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CTS742C083">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt;&lt;p&gt;
Source: http://www.ctscorp.com/components/Datasheets/CTSChipArrayDs.pdf</description>
</package>
</packages>
</library>
<library name="# stm32">
<description>ST Cortex-M3 STM32F101/103 processor family  in LQFP100, 64, 48 and VFQPFN36 pin versions</description>
<packages>
<package name="TQFP64">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="53047-04SMALL">
</package>
</packages>
</library>
<library name="# SerialPortBluetooth">
<packages>
<package name="BT_HC05_BASIC">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD110-R">
<description>&lt;b&gt;SOD110 Reflow soldering&lt;/b&gt; Philips SC01_Mounting_1996.pdf</description>
</package>
</packages>
</library>
<library name="transistor-pnp">
<description>&lt;b&gt;PNP Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-little-de">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="# jst">
<packages>
<package name="B3B-ZR">
<description>&lt;b&gt;JST ZH Connector&lt;/b&gt;
Top Entry type&lt;br&gt;
3 pol, 1.5 mm Pitch&lt;br&gt;
Source: &lt;a href="http://www.jst-mfg.com/product/pdf/eng/eZH.pdf"&gt;http://www.jst-mfg.com/product/pdf/eng/eZH.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP14" library="# SparkFun" package="1X03" value="MOT2"/>
<element name="C1" library="rcl" package="SMC_B" value="10u/20V">
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="IC9" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="BAT+" library="# stdlib" package="1X1_WITHOUT" value="">
<attribute name="VALUE"/>
</element>
<element name="BAT-" library="# stdlib" package="1X1_WITHOUT" value="">
<attribute name="VALUE"/>
</element>
<element name="IC10" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="IC11" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="R17" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0603" value="1.5k">
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="SMC_C" value="33u/20V">
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="# SparkFun2" package="1X04" value="SWD"/>
<element name="LED1" library="led" package="CHIPLED_0603" value="green">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0603" value="red">
<attribute name="VALUE"/>
</element>
<element name="SW1" library="# dp_devices" package="SW_TACT_3X6" value=""/>
<element name="JP1" library="SparkFun" package="USB-MINIB" value="USBMINIBSMD"/>
<element name="IC2" library="# SparkFun2" package="DPAK" value="NCP1117DT33G"/>
<element name="D2" library="# stdlib" package="SOD123W-DIODE" value="PMEG3010ER"/>
<element name="C3" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="SMC_A" value="10u/6.3V">
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-net" package="CTS742C083" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-net" package="CTS742C083" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="resistor-net" package="CTS742C083" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0603" value="22p">
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="22p">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="# stdlib" package="CRYTSAL-SMD-5X3" value="7B-8.000MAAJ-T"/>
<element name="R10" library="rcl" package="R0603" value="150">
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="1.5k">
<attribute name="VALUE"/>
</element>
<element name="JP13" library="# SparkFun" package="1X03" value="MOT1"/>
<element name="IC6" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="IC7" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="IC8" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="JP12" library="# SparkFun" package="1X03" value="MOT0"/>
<element name="IC3" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="IC4" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="IC5" library="# stdlib" package="DFN8" value="TC4452DFN08"/>
<element name="SW2" library="# dp_devices" package="SW_TACT_3X6" value=""/>
<element name="IC1" library="# stm32" package="TQFP64" value="STM32F103RCT6"/>
<element name="JP7" library="# SparkFun2" package="1X04" value="RC"/>
<element name="IC13" library="# SparkFun2" package="QFN-24" value="MPU6050"/>
<element name="R22" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0603" value="10n">
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0603" value="2.2n">
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="0">
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="0">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="# SparkFun2" package="1X03" value="UART"/>
<element name="R13" library="rcl" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="JP11" library="# SparkFun2" package="1X04" value="AUX"/>
<element name="R15" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="22">
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="22">
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="JP9" library="# SparkFun2" package="1X05" value="RC2"/>
<element name="JP10" library="# SparkFun2" package="1X02" value="BUT"/>
<element name="JP8" library="# SparkFun2" package="1X05" value="POT"/>
<element name="JP2" library="con-molex" package="53047-04SMALL" value="MPU-I2C#1"/>
<element name="C13" library="rcl" package="SMC_C" value="33u/20V">
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="IC14" library="# SerialPortBluetooth" package="BT_HC05_BASIC" value="BT HC06"/>
<element name="LED3" library="led" package="CHIPLED_0603" value="yellow">
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode" package="SOD110-R" value="1PS76SB40"/>
<element name="R1" library="rcl" package="R0603" value="47k">
<attribute name="VALUE"/>
</element>
<element name="T1" library="# stdlib" package="SO08" value="SI4835DDY"/>
<element name="JP4" library="# stdlib" package="MOLEX-53261-04-SMD-FLAT" value="I2C#2"/>
<element name="JP15" library="# SparkFun2" package="1X02" value="IR"/>
<element name="T2" library="transistor-pnp" package="SOT23" value="BCX71HSMD"/>
<element name="R19" library="rcl" package="R0603" value="2.2k">
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603" value="100n">
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0603" value="47">
<attribute name="VALUE"/>
</element>
<element name="IC12" library="74xx-little-de" package="SOT23-5" value="74AHC1G86DBV"/>
<element name="R16" library="rcl" package="R0603" value="10k">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="# jst" package="B3B-ZR" value="SPK"/>
<element name="D1" library="# stdlib" package="SOD123W-DIODE" value="PMEG3010ER"/>
<element name="SJ1" library="# SparkFun2" package="SJ_2S-TRACE" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="BAT-" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C12" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="IC9" pad="5"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC10" pad="5"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="3"/>
<contactref element="IC11" pad="5"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC11" pad="3"/>
<contactref element="C14" pad="-"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="C11" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="IC2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="RN3" pad="5"/>
<contactref element="RN1" pad="7"/>
<contactref element="RN3" pad="6"/>
<contactref element="RN3" pad="7"/>
<contactref element="RN2" pad="6"/>
<contactref element="RN2" pad="7"/>
<contactref element="RN1" pad="6"/>
<contactref element="RN1" pad="8"/>
<contactref element="RN1" pad="5"/>
<contactref element="RN2" pad="8"/>
<contactref element="RN2" pad="5"/>
<contactref element="RN3" pad="8"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="3"/>
<contactref element="JP7" pad="1"/>
<contactref element="IC13" pad="11"/>
<contactref element="IC13" pad="18"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="IC1" pad="63"/>
<contactref element="IC1" pad="18"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP10" pad="1"/>
<contactref element="JP8" pad="1"/>
<contactref element="C13" pad="-"/>
<contactref element="C23" pad="2"/>
<contactref element="IC14" pad="13"/>
<contactref element="IC14" pad="22"/>
<contactref element="LED3" pad="C"/>
<contactref element="JP2" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP15" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="JP4" pad="4"/>
<contactref element="IC13" pad="1"/>
<contactref element="IC12" pad="3"/>
<contactref element="R16" pad="1"/>
<contactref element="IC12" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC9" pad="1"/>
<contactref element="IC9" pad="8"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC10" pad="8"/>
<contactref element="IC11" pad="1"/>
<contactref element="IC11" pad="8"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="+"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC6" pad="8"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="C13" pad="+"/>
<contactref element="R17" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="T1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="M2A">
<contactref element="IC9" pad="6"/>
<contactref element="IC9" pad="7"/>
<contactref element="JP14" pad="1"/>
</signal>
<signal name="M2B">
<contactref element="IC10" pad="6"/>
<contactref element="IC10" pad="7"/>
<contactref element="JP14" pad="2"/>
</signal>
<signal name="A0">
<contactref element="IC3" pad="2"/>
<contactref element="RN1" pad="3"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="B0">
<contactref element="RN1" pad="2"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="C0">
<contactref element="IC5" pad="2"/>
<contactref element="RN1" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="3.3V">
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP5" pad="4"/>
<contactref element="IC2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="SW2" pad="1"/>
<contactref element="IC13" pad="13"/>
<contactref element="C19" pad="1"/>
<contactref element="IC13" pad="8"/>
<contactref element="C20" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="32"/>
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="64"/>
<contactref element="IC1" pad="19"/>
<contactref element="JP8" pad="5"/>
<contactref element="C23" pad="1"/>
<contactref element="IC14" pad="12"/>
<contactref element="JP2" pad="1"/>
<contactref element="T2" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="IC12" pad="5"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="22"/>
<contactref element="IC6" pad="2"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="B1">
<contactref element="IC7" pad="2"/>
<contactref element="RN2" pad="2"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="A2">
<contactref element="IC9" pad="2"/>
<contactref element="RN3" pad="3"/>
<contactref element="IC1" pad="62"/>
</signal>
<signal name="B2">
<contactref element="IC10" pad="2"/>
<contactref element="RN3" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="C2">
<contactref element="IC11" pad="2"/>
<contactref element="RN3" pad="2"/>
<contactref element="IC1" pad="61"/>
</signal>
<signal name="C1">
<contactref element="IC8" pad="2"/>
<contactref element="RN2" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SDA">
<contactref element="R15" pad="1"/>
<contactref element="IC1" pad="30"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="R14" pad="1"/>
<contactref element="IC1" pad="29"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="LIPO">
<contactref element="IC1" pad="21"/>
<contactref element="R18" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="TX">
<contactref element="R12" pad="1"/>
<contactref element="IC1" pad="51"/>
<contactref element="IC14" pad="2"/>
</signal>
<signal name="RX">
<contactref element="R13" pad="1"/>
<contactref element="IC1" pad="52"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="AUX0">
<contactref element="IC1" pad="35"/>
<contactref element="JP11" pad="2"/>
</signal>
<signal name="AUX1">
<contactref element="IC1" pad="36"/>
<contactref element="JP11" pad="3"/>
</signal>
<signal name="RC2">
<contactref element="IC1" pad="41"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="RC1/TX">
<contactref element="IC1" pad="42"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="RC0/RX">
<contactref element="IC1" pad="43"/>
<contactref element="IC12" pad="4"/>
</signal>
<signal name="LED0">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="LED1">
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="USB-D">
<contactref element="IC1" pad="57"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="M2C">
<contactref element="IC11" pad="7"/>
<contactref element="IC11" pad="6"/>
<contactref element="JP14" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="C11" pad="1"/>
<contactref element="SW1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="IC1" pad="60"/>
</signal>
<signal name="SWCLK">
<contactref element="IC1" pad="49"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="SWDIO">
<contactref element="IC1" pad="46"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="LED1" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED2" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="BOOT1">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="VUSB">
<contactref element="JP1" pad="VBUS"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="C9" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="C10" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="JP1" pad="D-"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="JP1" pad="D+"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="M1A">
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="7"/>
<contactref element="JP13" pad="1"/>
</signal>
<signal name="M1B">
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="7"/>
<contactref element="JP13" pad="2"/>
</signal>
<signal name="M1C">
<contactref element="IC8" pad="7"/>
<contactref element="IC8" pad="6"/>
<contactref element="JP13" pad="3"/>
</signal>
<signal name="M0A">
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="M0B">
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="7"/>
<contactref element="JP12" pad="2"/>
</signal>
<signal name="M0C">
<contactref element="IC5" pad="7"/>
<contactref element="IC5" pad="6"/>
<contactref element="JP12" pad="3"/>
</signal>
<signal name="USB-DM">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="44"/>
</signal>
<signal name="USB-DP">
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="45"/>
</signal>
<signal name="N$20">
<contactref element="IC13" pad="10"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC13" pad="20"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="JP6" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R12" pad="2"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="IC13" pad="9"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="RC2-0">
<contactref element="JP9" pad="2"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="RC2-1">
<contactref element="JP9" pad="3"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="RC2-3">
<contactref element="JP9" pad="5"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="RC2-2">
<contactref element="JP9" pad="4"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="BUT">
<contactref element="JP10" pad="2"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="SCL#2">
<contactref element="IC1" pad="58"/>
<contactref element="IC13" pad="23"/>
<contactref element="R23" pad="1"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="SDA#2">
<contactref element="IC1" pad="59"/>
<contactref element="IC13" pad="24"/>
<contactref element="R24" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="POT0">
<contactref element="JP8" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="POT1">
<contactref element="JP8" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="POT2">
<contactref element="JP8" pad="4"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$22">
<contactref element="R25" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="D3" pad="C"/>
<contactref element="IC14" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R1" pad="1"/>
<contactref element="T1" pad="4"/>
</signal>
<signal name="BATP">
<contactref element="BAT+" pad="1"/>
<contactref element="T1" pad="6"/>
<contactref element="T1" pad="5"/>
<contactref element="T1" pad="7"/>
<contactref element="T1" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="47"/>
</signal>
<signal name="N$26">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="GND1">
</signal>
<signal name="GND2">
</signal>
<signal name="GND3">
</signal>
<signal name="IR">
<contactref element="IC1" pad="14"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="T2" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="T2" pad="3"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R21" pad="2"/>
<contactref element="JP15" pad="2"/>
</signal>
<signal name="RC0-IN">
<contactref element="JP7" pad="2"/>
<contactref element="IC12" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="XOR">
<contactref element="IC1" pad="24"/>
<contactref element="R16" pad="2"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="+"/>
<contactref element="IC2" pad="3"/>
<contactref element="D2" pad="C"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="SJ1" pad="2"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC14" pad="24"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="AUX2">
<contactref element="IC1" pad="50"/>
<contactref element="JP11" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
