<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.635" x2="43.16" y2="0.635" width="0" layer="20"/>
<wire x1="43.16" y1="0.635" x2="43.16" y2="34.595" width="0" layer="20"/>
<wire x1="43.16" y1="34.595" x2="0" y2="34.595" width="0" layer="20"/>
<wire x1="0" y1="34.595" x2="0" y2="0.635" width="0" layer="20"/>
<text>9V | 10V</text>
<text>9V | 10V</text>
<text>Open
Hardware</text>
<text>Barbouri
2016</text>
<text>V-Ref Pwr
Board V1.0</text>
<text>Select jumper on J1 and J2 to select
5REF out of 9V 1-2 or 10V 2-3. Both
jumpers must match each other.</text>
<text>J1&amp;J2 must match</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="78LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="DUOLED-C-5MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green, red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
<package name="OSHW-LOGO-S_COPPER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5REF+" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5REF-" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BP1+" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BP1-" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BP2+" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BP2-" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="0.1uF"/>
<element name="C6" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FPS1" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FPS2" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="v-reg" package="78XXS" value="BA09C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="v-reg" package="78XXS" value="BA10T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="v-reg" package="78LXX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="DIP08" value="TINY85-20">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="LD1" library="led" package="DUOLED-C-5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="H2" library="holes" package="3,6" value="MOUNT-HOLE3.6"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S_COPPER" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="BP1-" pad="1"/>
<contactref element="BP2+" pad="1"/>
</signal>
<signal name="GND">
<contactref element="BP2-" pad="1"/>
<contactref element="IC1" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="5REF-" pad="1"/>
<contactref element="IC3" pad="GND"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IC2" pad="GND"/>
<contactref element="R4" pad="P$1"/>
<contactref element="U1" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="LD1" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="BP1+" pad="1"/>
<contactref element="FPS1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="FPS2" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="IC3" pad="IN"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="IC1" pad="IN"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="3"/>
<contactref element="IC2" pad="IN"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="OUT"/>
<contactref element="J1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="2"/>
<contactref element="5REF+" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="OUT"/>
<contactref element="J1" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="IC3" pad="OUT"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="P$2"/>
<contactref element="LD1" pad="AR"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$2"/>
<contactref element="LD1" pad="AX"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
