<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="10.16" y1="16.51" x2="55.88" y2="16.51" width="0" layer="20"/>
<wire x1="55.88" y1="16.51" x2="55.88" y2="57.14" width="0" layer="20"/>
<wire x1="55.88" y1="57.14" x2="10.16" y2="57.14" width="0" layer="20"/>
<wire x1="10.16" y1="57.14" x2="10.16" y2="16.51" width="0" layer="20"/>
<wire x1="27.94" y1="38.735" x2="45.72" y2="38.735" width="0.4064" layer="20"/>
<wire x1="45.72" y1="38.735" x2="45.72" y2="29.845" width="0.4064" layer="20"/>
<wire x1="45.72" y1="29.845" x2="27.94" y2="29.845" width="0.4064" layer="20"/>
<text>Big Purple Red Board</text>
<text>MDS 2014</text>
<text>GND</text>
<text>A1</text>
<text>B1</text>
<text>A2</text>
<text>B2</text>
<text>+5</text>
<text>GND</text>
<text>EN</text>
<text>STEP</text>
<text>DIR</text>
<text>Rev 4</text>
<text>V+</text>
<wire x1="27.94" y1="29.845" x2="27.94" y2="38.735" width="0.4064" layer="20"/>
<text>CUT OUT</text>
<text>63V</text>
<text>12-45V@3.5A</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>+5</text>
<text>GND</text>
<text>EN</text>
<text>STEP</text>
<text>DIR</text>
<text>+</text>
<text>_</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="1X08">
</package>
<package name="1X02">
</package>
<package name="2X3_SMT_POSTS">
<description>4UCON 15881&lt;br&gt;
Male .1" spaced SMT&lt;br&gt;
Keying posts into board</description>
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_H13">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="JP3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="M023.5MM"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-00809"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="PANASONIC_H13" value="100uF">
<attribute name="PROD_ID" value="CAP-08362"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STANDOFF1" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF2" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF3" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="STANDOFF4" library="SparkFun-Electromechanical" package="STAND-OFF" value="STAND-OFF"/>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="BSS84">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP8" library="SparkFun-Connectors" package="2X3_SMT_POSTS" value="">
<attribute name="PROD_ID" value="CONN-11415"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X05" value=""/>
</elements>
<signals>
<signal name="ENABLE">
<contactref element="JP1" pad="1"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="VMOT">
<contactref element="C1" pad="+"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="B2">
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="B1">
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="A1">
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="A2">
<contactref element="JP3" pad="4"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="FAULT">
<contactref element="Q2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="-"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="Q2" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP8" pad="5"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="M2">
<contactref element="JP1" pad="4"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="M1">
<contactref element="JP1" pad="3"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="M0">
<contactref element="JP1" pad="2"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="DIR">
<contactref element="JP1" pad="8"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="STEP">
<contactref element="JP1" pad="7"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
