<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="19.05" y2="25.4" width="0" layer="20"/>
<wire x1="19.05" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>RTS</text>
<text>TXO</text>
<text>RXI</text>
<text>VIN</text>
<text>GND</text>
<text>Bluetooth LE
Serial Interface</text>
<text>digitalmisery.com</text>
<text>CTS</text>
<text>CONN</text>
<text>BLE
LINK</text>
<text>RTS</text>
<text>LINK</text>
<text>PIN 6</text>
<text>PIN 2</text>
<text>CTS</text>
<text>INT</text>
<text>GROUND CTS
IF NO FLOW
CONTROL</text>
<text>VIN = 
3.3-6V</text>
<text>3.3V</text>
<text>BLE112</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="1X06-CLEANBIG">
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BLE112-A">
<description>BLE112-A&lt;BR&gt;
Bluetooth 4.0 module with built-in chip antenna.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="nonolith">
<packages>
<package name="SOT23-3">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="_ohw-logo">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
<library name="Tag-Connect">
<packages>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="SparkFun-RF" package="BLE112-A" value="BLE112-A"/>
<element name="C4" library="adafruit" package="C0805K" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805K" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805K" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="nonolith" package="SOT23-3" value="MCP1700">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="_ohw-logo" package="OSHW_FILLX150_NOTEXT" value=""/>
<element name="JP1" library="adafruit" package="1X06-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="Tag-Connect" package="TC2030-MCP-NL" value=""/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ_2" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="LED" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="10"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="21"/>
<contactref element="U2" pad="30"/>
<contactref element="U2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="9"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="20"/>
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="P0_0">
<contactref element="U2" pad="28"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="P1_0">
<contactref element="U2" pad="18"/>
</signal>
<signal name="P2_1">
<contactref element="U2" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="P2_2">
<contactref element="U2" pad="4"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="TXO">
<contactref element="U2" pad="24"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RXI">
<contactref element="U2" pad="23"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="LED" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="BTWAKE">
<contactref element="U2" pad="8"/>
</signal>
<signal name="BTRES">
<contactref element="U2" pad="29"/>
<contactref element="J1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$6">
</signal>
<signal name="CTS">
<contactref element="U2" pad="26"/>
<contactref element="SJ2" pad="3"/>
</signal>
<signal name="RTS">
<contactref element="U2" pad="25"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="P1_7">
<contactref element="U2" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PIN6">
<contactref element="JP1" pad="6"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="PIN2">
<contactref element="SJ2" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="P0_1">
<contactref element="U2" pad="27"/>
<contactref element="SJ2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
