<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="116.84" x2="0" y2="121.92" width="0.1524" layer="20"/>
<wire x1="0" y1="121.92" x2="2.54" y2="124.46" width="0.1524" layer="20" curve="-90"/>
<wire x1="2.54" y1="124.46" x2="5.08" y2="124.46" width="0.1524" layer="20"/>
<wire x1="5.08" y1="124.46" x2="27.94" y2="124.46" width="0.1524" layer="20"/>
<wire x1="27.94" y1="124.46" x2="30.48" y2="124.46" width="0.1524" layer="20"/>
<wire x1="30.48" y1="124.46" x2="33.02" y2="121.92" width="0.1524" layer="20" curve="-90"/>
<wire x1="33.02" y1="121.92" x2="33.02" y2="116.84" width="0.1524" layer="20"/>
<wire x1="33.02" y1="116.84" x2="33.02" y2="78.74" width="0.1524" layer="20"/>
<wire x1="33.02" y1="78.74" x2="35.56" y2="76.2" width="0.1524" layer="20" curve="90"/>
<wire x1="35.56" y1="76.2" x2="48.26" y2="76.2" width="0.1524" layer="20"/>
<wire x1="48.26" y1="76.2" x2="50.8" y2="73.66" width="0.1524" layer="20" curve="-90"/>
<wire x1="50.8" y1="73.66" x2="50.8" y2="17.78" width="0.1524" layer="20"/>
<wire x1="50.8" y1="17.78" x2="48.26" y2="15.24" width="0.1524" layer="20" curve="-90"/>
<wire x1="48.26" y1="15.24" x2="2.54" y2="15.24" width="0.1524" layer="20"/>
<wire x1="2.54" y1="15.24" x2="0" y2="17.78" width="0.1524" layer="20" curve="-90"/>
<wire x1="0" y1="17.78" x2="0" y2="116.84" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="Particle-Devices">
<description>&lt;h3&gt;Reference foot prints for Particle devices&lt;/h3&gt;
In this library you'll find foot prints to make circuit boards using the Particle devices: Spark Core, Photon and Electron.&lt;br&gt;&lt;br&gt;
There are for reference and you may need to adjust them for your application. See https://docs.particle.io for more details on the recommended layouts for Particle devices.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Designed by Particle. Distributed under a Creative Commons Attribution, Share-Alike license. Development kits based on this library should be distributed under a similar license. Commercial products using this library as a reference design need not comply with this license; further questions can be sent to hello@particle.io. Check license.txt for more information.</description>
<packages>
<package name="ELECTRON">
</package>
<package name="E0">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Particle-Devices" package="ELECTRON" value="ELECTRON_WITH_HEADERS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Particle-Devices" package="E0" value="E0_V005"/>
</elements>
<signals>
<signal name="VBAT">
<contactref element="U1" pad="11"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="C0">
<contactref element="U1" pad="49"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="C1">
<contactref element="U1" pad="48"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="42"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="41"/>
<contactref element="U$1" pad="26"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="40"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="39"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="38"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="37"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="36"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="35"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="17"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="16"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="51"/>
<contactref element="U1" pad="58"/>
<contactref element="U1" pad="60"/>
<contactref element="U1" pad="59"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="33"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="9"/>
<contactref element="U$1" pad="36"/>
</signal>
<signal name="C2">
<contactref element="U1" pad="47"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="C3">
<contactref element="U1" pad="46"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="C4">
<contactref element="U1" pad="45"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="C5">
<contactref element="U1" pad="44"/>
<contactref element="U$1" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
