<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.81" y2="0" width="0" layer="20"/>
<wire x1="48.81" y1="0" x2="48.81" y2="42.03" width="0" layer="20"/>
<wire x1="48.81" y1="42.03" x2="0" y2="42.03" width="0" layer="20"/>
<wire x1="0" y1="42.03" x2="0" y2="0" width="0" layer="20"/>
<text>SHDN</text>
<text>DIN</text>
<text>DOUT</text>
<text>SCLK</text>
<text>BATT</text>
<text>-</text>
<text>PANEL</text>
<text>Ft. Sumter SHM Rev. B
Accelerometer Breakout
Clemson University</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>BATTV/2</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>BATTV/2</text>
<text>GND</text>
<text>DIN</text>
<text>DOUT</text>
<text>SHDN</text>
<text>SCLK</text>
<text>Ft. Sumter SHM Rev. B
Accelerometer Breakout
Clemson University</text>
<text>PANEL</text>
<text>-</text>
<text>+</text>
<text>BATT</text>
<text>-</text>
<text>+</text>
</plain>
<libraries>
<library name="josiahlib">
<packages>
<package name="10-VSSOP">
</package>
<package name="CDRHSMD">
</package>
<package name="LCC20">
<description>&lt;b&gt;LCC 20&lt;/b&gt; Leadless Chip Carrier &lt;p&gt; Ceramic Package</description>
</package>
<package name="SC-82AB">
</package>
<package name="MAX1795-8LUMAX">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DO-216AA">
<description>&lt;b&gt;Manufacturer&lt;/b&gt;:
Microsemi Commercial Components Group&lt;br&gt;
&lt;b&gt;Package: &lt;/b&gt;DO-216AA&lt;br&gt;

Fits UPS115UE3/TR7: DIODE SCHOTTKY 15V 1A POWERMITE</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ADC" library="josiahlib" package="10-VSSOP" value="ADS1118IDGST"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="47uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="L1" library="josiahlib" package="CDRHSMD" value="10uH"/>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.01uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="L2" library="SparkFun-Passives" package="0603" value="2.5kOhm@100MHz"/>
<element name="ACCELL" library="josiahlib" package="LCC20" value="MODEL1521ACCEL"/>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="5k">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="5k">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.01uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="U$2" library="holes" package="3,0" value=""/>
<element name="U$3" library="holes" package="3,0" value=""/>
<element name="U$4" library="holes" package="3,0" value=""/>
<element name="BATTERY" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK"/>
<element name="SOLAR_PANEL" library="SparkFun-Connectors" package="1X02_LOCK" value="M02LOCK"/>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="3V_REGULATOR" library="josiahlib" package="SC-82AB" value="NCP583SQ30T1G"/>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="0.01uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="SparkFun-Passives" package="0603" value="2.5kOhm@100MHz">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="PROD_ID" value="CAP-10057"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="0.01uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="L4" library="SparkFun-Passives" package="0603" value="2.5kOhm@100MHz"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DO-216AA" value="DIODE-SCHOTTKYUPS115UE3/TR7">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1MΩ">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1MΩ">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="STEPUP" library="josiahlib" package="MAX1795-8LUMAX" value="MAX1795"/>
<element name="C16" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="5k">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="5k">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ADC" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="ACCELL" pad="18"/>
<contactref element="ACCELL" pad="19"/>
<contactref element="ACCELL" pad="6"/>
<contactref element="ACCELL" pad="5"/>
<contactref element="ACCELL" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="3V_REGULATOR" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="BATTERY" pad="2"/>
<contactref element="ADC" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="SOLAR_PANEL" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="STEPUP" pad="2"/>
<contactref element="STEPUP" pad="5"/>
<contactref element="STEPUP" pad="1"/>
<contactref element="STEPUP" pad="3"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="DOUT">
<contactref element="ADC" pad="10"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="ACCELL" pad="12"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="ACCELL" pad="16"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="L1" pad="P$2"/>
<contactref element="STEPUP" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="STEPUP" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="ACCELL" pad="17"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="5V">
<contactref element="ACCELL" pad="9"/>
<contactref element="ACCELL" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="ACCELL" pad="11"/>
<contactref element="ACCELL" pad="14"/>
<contactref element="R1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="DIN">
<contactref element="ADC" pad="9"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="VREG">
<contactref element="C2" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="STEPUP" pad="8"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="SHDN">
<contactref element="JP2" pad="3"/>
<contactref element="STEPUP" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="C8" pad="1"/>
<contactref element="3V_REGULATOR" pad="3"/>
<contactref element="C11" pad="1"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="BATT+">
<contactref element="BATTERY" pad="1"/>
<contactref element="3V_REGULATOR" pad="4"/>
<contactref element="C9" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="2"/>
<contactref element="3V_REGULATOR" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ADC" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="C1" pad="1"/>
<contactref element="ADC" pad="8"/>
<contactref element="C14" pad="1"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="PANEL+">
<contactref element="SOLAR_PANEL" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="BATTERY">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="AIN1">
<contactref element="ADC" pad="5"/>
<contactref element="R5" pad="2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="AIN0">
<contactref element="ADC" pad="4"/>
<contactref element="R6" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
