<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.2">
<drawing>
<board>
<plain>
<wire x1="-21.4122" y1="-0.1016" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="25.4" width="0" layer="20"/>
<wire x1="25.4" y1="25.4" x2="-21.4122" y2="25.2984" width="0" layer="20"/>
<wire x1="-21.4122" y1="25.2984" x2="-21.4122" y2="-0.1016" width="0" layer="20"/>
<text>100</text>
<text>1M</text>
<text>Br-Bk-Br</text>
<text>Br-Bk-Gr</text>
<text>BEAST Board</text>
<text>BEAST
Robotics
2202</text>
<text>STEM
Camp</text>
<text>100</text>
<text>Br-Bk-Br</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="CE28XX">
<packages>
<package name="PS12">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08_MCU">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="BS-7">
<packages>
<package name="BAT_BS-7">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="CE28XX" package="PS12" value="PS12PIEZO">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE" value="1k"/>
</element>
<element name="U1" library="SparkFun-Retired" package="DIP08_MCU" value="TINY45-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09439"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08380"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="3" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="5" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
<element name="BT1" library="BS-7" package="BAT_BS-7" value="BS-7">
<attribute name="DESCRIPTION" value=" Battery Holder (Open) Coin, 20.0mm 1 Cell PC Pin "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="BS-7-ND"/>
<attribute name="MF" value="MPD (Memory"/>
<attribute name="MP" value="BS-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/BS-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="6"/>
<contactref element="P1" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="P$2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="8"/>
<contactref element="BT1" pad="+"/>
</signal>
<signal name="GND">
<contactref element="P1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="D1" pad="K"/>
<contactref element="R2" pad="P$1"/>
<contactref element="D2" pad="K"/>
<contactref element="BT1" pad="-"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="5"/>
<contactref element="5" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
