<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="28.88" y2="0" width="0" layer="20"/>
<wire x1="28.88" y1="0" x2="28.88" y2="69.84" width="0" layer="20"/>
<wire x1="28.88" y1="69.84" x2="1.27" y2="69.84" width="0" layer="20"/>
<wire x1="1.27" y1="69.84" x2="1.27" y2="0" width="0" layer="20"/>
<text>I AM</text>
<text>Green: OK
Red: NOT OK
Yellow:
   It's complicated.</text>
<text>Feelings Indicator 0.2
by Giles Cooper</text>
</plain>
<libraries>
<library name="BC2032-E2">
<packages>
<package name="MPD_BC2032-E2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MMRGB">
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
</packages>
</library>
<library name="1825910-6">
<packages>
<package name="SW_1825910-6-4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR-2032" library="BC2032-E2" package="MPD_BC2032-E2" value="BC2032-E2">
<attribute name="DESCRIPTION" value=" Holder Battery Cr2032 Sony Equal "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="BC2032-E2-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/mpd-memory-protection-devices/BC2032-E2/BC2032-E2-ND/2077836?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="MPD _Memory"/>
<attribute name="MP" value="BC2032-E2"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DFN-8 Memory Protection Devices"/>
</element>
<element name="LED5MMRGB" library="adafruit" package="LED5MMRGB" value="RGBLED_CA-5MM">
<attribute name="NAME"/>
</element>
<element name="220Ω" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2200Ω" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="1825910-6" package="SW_1825910-6-4" value="1825910-6">
<attribute name="COMMENT" value="1825910-6"/>
<attribute name="CONFIGURATION_POLE-THROW" value="Single Pole - Single Throw"/>
<attribute name="CONTACT_CURRENT_RATING" value="50 mA"/>
<attribute name="DESCRIPTION" value=" FSM4JH=6MM TACT SWITCH, HIGH TEMP "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="450-1650-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/te-connectivity-alcoswitch-switches/1825910-6/450-1650-ND/1632536?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1825910-6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="TE_PURCHASE_URL" value="https://www.te.com/usa-en/product-1825910-6.html?te_bu=Cor&amp;te_type=disp&amp;te_campaign=seda_glo_cor-seda-global-disp-prtnr-fy19-seda-model-bom-cta_sma-317_1&amp;elqCampaignId=32493"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="1825910-6" package="SW_1825910-6-4" value="1825910-6">
<attribute name="COMMENT" value="1825910-6"/>
<attribute name="CONFIGURATION_POLE-THROW" value="Single Pole - Single Throw"/>
<attribute name="CONTACT_CURRENT_RATING" value="50 mA"/>
<attribute name="DESCRIPTION" value=" FSM4JH=6MM TACT SWITCH, HIGH TEMP "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="450-1650-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/te-connectivity-alcoswitch-switches/1825910-6/450-1650-ND/1632536?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="1825910-6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="TE_PURCHASE_URL" value="https://www.te.com/usa-en/product-1825910-6.html?te_bu=Cor&amp;te_type=disp&amp;te_campaign=seda_glo_cor-seda-global-disp-prtnr-fy19-seda-model-bom-cta_sma-317_1&amp;elqCampaignId=32493"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="CR-2032" pad="N"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="2200Ω" pad="2"/>
<contactref element="LED5MMRGB" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="LED5MMRGB" pad="1"/>
<contactref element="220Ω" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LED5MMRGB" pad="2"/>
<contactref element="CR-2032" pad="P"/>
</signal>
<signal name="N$2">
<contactref element="2200Ω" pad="1"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="220Ω" pad="1"/>
<contactref element="SW2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
