<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="88.57" y2="0" width="0" layer="20"/>
<wire x1="88.57" y1="0" x2="88.57" y2="45.71" width="0" layer="20"/>
<wire x1="88.57" y1="45.71" x2="0" y2="45.71" width="0" layer="20"/>
<wire x1="0" y1="45.71" x2="0" y2="0" width="0" layer="20"/>
<text>&gt;REVISION</text>
<text>https://retro.moe</text>
<text>REV</text>
<text>UniJoystiCle</text>
<text>2016/06/20</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="POWER_JACK_SLOT">
</package>
</packages>
</library>
<library name="ESP12E_DEVKIT">
<packages>
<package name="ESP12E_DEVKIT">
<description>ESP12E_DEVKIT</description>
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REVISION" value="0.2.2"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="DO41-10" value="1N4001">
<attribute name="MPN" value="1N4001"/>
<attribute name="MF" value="NTE ELECTRONICS"/>
<attribute name="OC_NEWARK" value="10M8464"/>
<attribute name="NAME"/>
</element>
<element name="IC1" library="40xx" package="DIL14" value="4066N">
<attribute name="MPN" value="SN74HC4066N"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_NEWARK" value="76C3574"/>
<attribute name="NAME"/>
</element>
<element name="IC2" library="40xx" package="DIL14" value="4066N">
<attribute name="MPN" value="SN74HC4066N"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_NEWARK" value="76C3574"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="40xx" package="DIL14" value="4066N">
<attribute name="MPN" value="SN74HC4066N"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_NEWARK" value="76C3574"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="DB9" value="DB9">
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="16T0655"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="618009231121"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="DB9" value="DB9">
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="16T0655"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="618009231121"/>
</element>
<element name="MOD1" library="ESP12E_DEVKIT" package="ESP12E_DEVKIT" value="ESP12E_DEVKIT">
<attribute name="NAME"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="POWER_JACK_SLOT" value="POWER_JACKSLT">
<attribute name="PROD_ID" value="PRT-00119"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="J1UP">
<contactref element="IC1" pad="13"/>
<contactref element="MOD1" pad="D0"/>
</signal>
<signal name="J1DOWN">
<contactref element="IC1" pad="5"/>
<contactref element="MOD1" pad="D1"/>
</signal>
<signal name="J1LEFT">
<contactref element="IC1" pad="6"/>
<contactref element="MOD1" pad="D2"/>
</signal>
<signal name="J1RIGHT">
<contactref element="IC1" pad="12"/>
<contactref element="MOD1" pad="D3"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="8"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="11"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="IC3" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="4"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="IC3" pad="8"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="IC3" pad="11"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="7"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC2" pad="7"/>
<contactref element="MOD1" pad="GND@3"/>
<contactref element="J2" pad="8"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC2" pad="3"/>
<contactref element="J1" pad="8"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="7"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC3" pad="14"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$21">
<contactref element="IC2" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="4"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$23">
<contactref element="D1" pad="A"/>
<contactref element="J3" pad="PWR"/>
</signal>
<signal name="5V">
<contactref element="D1" pad="C"/>
<contactref element="MOD1" pad="VIN"/>
</signal>
<signal name="3.3V">
<contactref element="MOD1" pad="GND@1"/>
<contactref element="J3" pad="GND@1"/>
<contactref element="J3" pad="GND@2"/>
</signal>
<signal name="J1FIRE">
<contactref element="IC2" pad="13"/>
<contactref element="MOD1" pad="D4"/>
</signal>
<signal name="J2UP">
<contactref element="MOD1" pad="D5"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="J2DOWN">
<contactref element="MOD1" pad="D6"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="J2LEFT">
<contactref element="MOD1" pad="D7"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="J2RIGHT">
<contactref element="MOD1" pad="D8"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="J2FIRE">
<contactref element="MOD1" pad="RX"/>
<contactref element="IC2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
