<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="11.049" y1="7.937" x2="12.192" y2="7.937" width="0" layer="20"/>
<wire x1="12.192" y1="7.937" x2="12.192" y2="6.477" width="0" layer="20"/>
<wire x1="12.192" y1="6.477" x2="16.51" y2="6.477" width="0" layer="20"/>
<wire x1="0.254" y1="4.953" x2="0.254" y2="7.62" width="0" layer="20"/>
<wire x1="0.254" y1="7.62" x2="2.54" y2="7.62" width="0" layer="20"/>
<wire x1="2.54" y1="7.62" x2="2.54" y2="6.477" width="0" layer="20"/>
<wire x1="11.049" y1="7.937" x2="11.049" y2="6.477" width="0" layer="20"/>
<wire x1="11.049" y1="6.477" x2="2.54" y2="6.477" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="2.54" y2="4.953" width="0" layer="20"/>
<wire x1="2.54" y1="4.953" x2="0.254" y2="4.953" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="16.51" y1="6.477" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="3.556" x2="15.24" y2="2.032" width="0.9906" layer="46"/>
<wire x1="3.81" y1="3.556" x2="3.81" y2="2.032" width="0.9906" layer="46"/>
<text>github.com/thatdecade</text>
<text>/gba-sp-usb-c</text>
<text>5.1k</text>
<text>UJC-VP-3-SMT-TR</text>
<text>FACEDOWN</text>
</plain>
<libraries>
<library name="UJC-VP-3-SMT-TR">
<packages>
<package name="CUI_UJC-VP-3-SMT-TR">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-TIGHT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="UJC-VP-3-SMT-TR" package="CUI_UJC-VP-3-SMT-TR" value="UJC-VP-3-SMT-TR">
<attribute name="MAXIMUM_PACKAGE_HEIGHT" value="6.5mm"/>
<attribute name="MANUFACTURER" value="CUI Devices"/>
<attribute name="STANDARD" value="Manufacturer Recommendations"/>
<attribute name="PARTREV" value="1.0"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0402-TIGHT" value="5.1k">
<attribute name="PROD_ID" value="RES-14340"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0402-TIGHT" value="5.1k">
<attribute name="PROD_ID" value="RES-14340"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="A12"/>
<contactref element="J1" pad="B12"/>
<contactref element="J1" pad="S1B"/>
<contactref element="J1" pad="S1A"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="S2A"/>
<contactref element="J1" pad="S2B"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="B5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="A5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="J1" pad="B9"/>
<contactref element="J1" pad="A9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
