<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.907" y2="0" width="0" layer="20"/>
<wire x1="17.907" y1="0" x2="17.907" y2="13.208" width="0" layer="20"/>
<wire x1="17.907" y1="13.208" x2="15.224" y2="13.208" width="0" layer="20"/>
<wire x1="15.224" y1="13.208" x2="15.224" y2="35.687" width="0" layer="20"/>
<wire x1="15.224" y1="35.687" x2="2.683" y2="35.687" width="0" layer="20"/>
<wire x1="2.683" y1="35.687" x2="2.683" y2="13.208" width="0" layer="20"/>
<wire x1="2.683" y1="13.208" x2="0" y2="13.208" width="0" layer="20"/>
<wire x1="0" y1="13.208" x2="0" y2="0" width="0" layer="20"/>
<text>LS SMARTSTICK</text>
<text>REV6</text>
<text>JWKR</text>
<text>VUSB</text>
<text>3V3</text>
<text>23</text>
<text>22</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>GND</text>
<text>VIN</text>
<text>A10</text>
<text>Q2</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
</package>
<package name="1X01NS">
</package>
</packages>
</library>
<library name="smartsticks">
<packages>
<package name="JST-2-PTH-2">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-4-PTH">
<description>&lt;h3&gt;JST Right Angle 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PTS645VH83-2LFS">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="AO3401A">
<description>&lt;30V P-Channel MOSFET&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X125-3N">
<description>&lt;b&gt;SOT-23-3L&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="LiPoChargerTeensy3.1.v04a">
<description>Generated from &lt;b&gt;LiPoChargerTeensy3.1.v04a.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="KRIS_STBC08">
<description>STBC08 800 mA standalone LiPo battery charger</description>
</package>
</packages>
</library>
<library name="Smartstick.rev6">
<description>Generated from &lt;b&gt;Smartstick.rev3.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="436331045822">
<description>WS-TUS-3.5x4.7 mm side push SMD Tact Switch with boss design, 4 pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY_VUSB_AGND" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="TEENSY_VIN" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="TEENSY_PIN0_GND" library="SparkFun-Connectors" package="1X02_NO_SILK" value="M021X02_NO_SILK"/>
<element name="TEENSY_PIN_1" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="TEENSY_3V3" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="J1" library="smartsticks" package="JST-2-PTH-2" value="BATT_JST">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09863"/>
<attribute name="SKU" value="PRT-09914"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="smartsticks" package="JST-4-PTH" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="WIRE-13531"/>
<attribute name="SF_ID" value="PRT-09916"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY_PIN_2" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="TEENSY_PIN_23" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="GND" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="SW3" library="smartsticks" package="PTS645VH83-2LFS" value="PTS645VH83-2LFS">
<attribute name="VALUE"/>
</element>
<element name="ANCHOR1" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="TEENSY_PROGRAM" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS">
<attribute name="SPICEPREFIX" value="X"/>
</element>
<element name="TEENSY_PIN_3" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="TEENSY_PIN_22" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="3M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="AO3401A" package="SOT95P280X125-3N" value="AO3401A">
<attribute name="DESCRIPTION" value="30V P-Channel MOSFET"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="MANUFACTURER_NAME" value="Alpha &amp; Omega Semiconductors"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AO3401A"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="LiPoChargerTeensy3.1.v04a" package="KRIS_STBC08" value="KRIS_STBC08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="1250">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="TEENSY_PIN_A10" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="AO3401A" package="SOT95P280X125-3N" value="AO3401A">
<attribute name="DESCRIPTION" value="30V P-Channel MOSFET"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="MANUFACTURER_NAME" value="Alpha &amp; Omega Semiconductors"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AO3401A"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07853"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="Smartstick.rev6" package="436331045822" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="P$7"/>
<contactref element="U2" pad="P$4"/>
<contactref element="R4" pad="1"/>
<contactref element="TEENSY_PIN0_GND" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="SW3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="3"/>
<contactref element="TEENSY_PIN_3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="TEENSY_PIN_A10" pad="1"/>
</signal>
<signal name="LEDV">
<contactref element="J2" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="VUSB">
<contactref element="TEENSY_VUSB_AGND" pad="1"/>
<contactref element="U2" pad="P$6"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="P$1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="P$5"/>
</signal>
<signal name="N$6">
<contactref element="TEENSY_PIN_22" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="TEENSY_VUSB_AGND" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Q2" pad="3"/>
<contactref element="TEENSY_VIN" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="Q2" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U2" pad="P$3"/>
<contactref element="TEENSY_PIN_23" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="TEENSY_PIN0_GND" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="SW3" pad="1"/>
<contactref element="TEENSY_PIN_2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="TEENSY_PIN_1" pad="1"/>
<contactref element="U2" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
