<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="7.62" x2="2.54" y2="7.62" width="0" layer="20"/>
<wire x1="2.54" y1="7.62" x2="0" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="0" y1="5.08" x2="2.54" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="2.54" x2="5.08" y2="2.54" width="0" layer="20"/>
<wire x1="5.08" y1="2.54" x2="5.08" y2="0.3175" width="0" layer="20"/>
<wire x1="5.08" y1="0.3175" x2="5.3975" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.3975" y1="0" x2="14.903125" y2="0" width="0" layer="20"/>
<wire x1="14.903125" y1="0" x2="15.220625" y2="0.3175" width="0" layer="20" curve="90"/>
<wire x1="15.220625" y1="0.3175" x2="15.239375" y2="9.8425" width="0" layer="20"/>
<wire x1="15.239375" y1="9.8425" x2="14.921875" y2="10.16" width="0" layer="20" curve="90.112787"/>
<wire x1="14.921875" y1="10.16" x2="5.3975" y2="10.16" width="0" layer="20"/>
<wire x1="5.3975" y1="10.16" x2="5.08" y2="9.8425" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="9.8425" x2="5.08" y2="7.62" width="0" layer="20"/>
<text>GND</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="E2,5-5" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="2X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="+"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP4" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="JP4" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="JP4" pad="4"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="7"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
