<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>f.lux</text>
<text>Bad Wolf Robotics</text>
<text>Created by Bryson Reece</text>
<text>No animals were harmed in the making of this shield</text>
<text>1</text>
<text>14</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="ARDUINOR3">
<description>The new Arduino R3 'classic' adds duplicate I2C pins and an IORef pin (and an unused pin</description>
</package>
<package name="OSHWLOGO_TOP_0.2">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2051">
<description>.100" (2.54mm) Center Header - 5 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="adafruit" package="ARDUINOR3" value="ARDUINOR3-DIMENSION"/>
<element name="X1" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X2" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X3" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X4" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X5" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X6" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X7" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X8" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X9" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X10" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X11" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X12" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X13" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="X14" library="con-molex" package="22-23-2051" value="22-23-2051">
<attribute name="OC_NEWARK" value="38C9178"/>
<attribute name="MPN" value="22-23-2051"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462952"/>
</element>
<element name="U$1" library="adafruit" package="OSHWLOGO_TOP_0.2" value=""/>
</elements>
<signals>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="GND1">
<contactref element="U1" pad="GND1"/>
</signal>
<signal name="GND2">
<contactref element="U1" pad="GND2"/>
</signal>
<signal name="3V">
<contactref element="U1" pad="3V"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="5V"/>
<contactref element="X8" pad="1"/>
<contactref element="X9" pad="1"/>
<contactref element="X10" pad="1"/>
<contactref element="X11" pad="1"/>
<contactref element="X12" pad="1"/>
<contactref element="X13" pad="1"/>
<contactref element="X14" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="X4" pad="1"/>
<contactref element="X5" pad="1"/>
<contactref element="X6" pad="1"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="X8" pad="4"/>
<contactref element="X9" pad="4"/>
<contactref element="X10" pad="4"/>
<contactref element="X11" pad="4"/>
<contactref element="X12" pad="4"/>
<contactref element="X13" pad="4"/>
<contactref element="X14" pad="4"/>
<contactref element="X1" pad="4"/>
<contactref element="X2" pad="4"/>
<contactref element="X4" pad="4"/>
<contactref element="X5" pad="4"/>
<contactref element="X6" pad="4"/>
<contactref element="X7" pad="4"/>
<contactref element="X3" pad="4"/>
<contactref element="U1" pad="GND"/>
</signal>
<signal name="N$4">
<contactref element="X8" pad="5"/>
<contactref element="X9" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="X9" pad="5"/>
<contactref element="X10" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="X11" pad="3"/>
<contactref element="X10" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="X11" pad="5"/>
<contactref element="X12" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="X13" pad="3"/>
<contactref element="X12" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="X14" pad="3"/>
<contactref element="X13" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="X8" pad="3"/>
<contactref element="X7" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="X1" pad="5"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="X2" pad="5"/>
<contactref element="X3" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="X3" pad="5"/>
<contactref element="X4" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="X4" pad="5"/>
<contactref element="X5" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="X6" pad="3"/>
<contactref element="X5" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="X6" pad="5"/>
<contactref element="X7" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="D6"/>
<contactref element="X1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
