<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="7.62" y1="0" x2="66.04" y2="0" width="0" layer="20"/>
<wire x1="66.04" y1="0" x2="66.04" y2="22.86" width="0" layer="20"/>
<wire x1="66.04" y1="22.86" x2="7.62" y2="22.86" width="0" layer="20"/>
<wire x1="7.62" y1="22.86" x2="7.62" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>U3s Low Pass Filter Test Fixture</text>
<text>U3s Low Pass Filter Test Fixture</text>
<text>INPUT</text>
<text>OUTPUT</text>
<text>INPUT</text>
<text>OUTPUT</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LTI-SASF54GT">
<description>&lt;b&gt;SMA vertical PCB thrue hole jack&lt;/b&gt;&lt;p&gt;
Source: Lighthorse Technologies, inc. SASF54GT.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN" library="SparkFun-Connectors" package="1X04" value="IN">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="OUT">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-coax" package="LTI-SASF54GT" value="LTI-SASF54GT">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X2" library="con-coax" package="LTI-SASF54GT" value="LTI-SASF54GT">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IN" pad="4"/>
<contactref element="IN" pad="3"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="3"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="5"/>
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="3"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="IN" pad="1"/>
<contactref element="IN" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="X2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
