<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<wire x1="5.54" y1="2.41" x2="64.58" y2="2.41" width="0" layer="20"/>
<wire x1="67.67" y1="5.48" x2="67.68" y2="29.55" width="0" layer="20"/>
<wire x1="64.54" y1="32.67" x2="5.44" y2="32.67" width="0" layer="20"/>
<wire x1="5.44" y1="32.67" x2="5.43" y2="32.67" width="0" layer="20"/>
<wire x1="2.4" y1="29.58" x2="2.4" y2="5.49" width="0" layer="20"/>
<text>GND</text>
<text>PWR</text>
<text>ID</text>
<text>L1</text>
<text>L4</text>
<text>L2</text>
<text>L3</text>
<text>LCOM</text>
<text>TCOM</text>
<text>T1</text>
<text>T2</text>
<text>T3</text>
<text>T4</text>
<text>Michael Kroll 
Dec. 3rd, 2017</text>
<text>Feller 
3914-1-FMI-L-P-61
RPI HAT</text>
<wire x1="5.54" y1="2.41" x2="2.4" y2="5.49" width="0" layer="20" curve="-88.89465"/>
<wire x1="64.58" y1="2.41" x2="67.67" y2="5.48" width="0" layer="20" curve="89.627942"/>
<wire x1="64.54" y1="32.67" x2="67.68" y2="29.54" width="0" layer="20" curve="-91.671399"/>
<wire x1="2.4" y1="29.58" x2="5.44" y2="32.67" width="0" layer="20" curve="-89.065318"/>
</plain>
<libraries>
<library name="RPI-Zero">
<description>Generated from &lt;b&gt;TMC2660-test-with-grbl.brd&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="RPI-Zero" package="RASPBERRYPI_BASTELSTUBE_V13_RASPI_BOARD_B+_FULL" value="RPI-ZERO"/>
<element name="J1" library="SparkFun-Connectors" package="1X05" value="Taster">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05" value="LEDs">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03" value="System">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
</elements>
<signals>
<signal name="L1">
<contactref element="J2" pad="2"/>
<contactref element="U$1" pad="40"/>
</signal>
<signal name="L2">
<contactref element="J2" pad="3"/>
<contactref element="U$1" pad="38"/>
</signal>
<signal name="L3">
<contactref element="J2" pad="4"/>
<contactref element="U$1" pad="36"/>
</signal>
<signal name="L4">
<contactref element="J2" pad="5"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="T1">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="T2">
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="T3">
<contactref element="J1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="T4">
<contactref element="J1" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="ID">
<contactref element="J3" pad="1"/>
<contactref element="U$1" pad="37"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="2"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="39"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="30"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="6"/>
<contactref element="J2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="POWER">
<contactref element="J3" pad="3"/>
<contactref element="U$1" pad="35"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="17"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="5V0">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
