<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.6" y2="0" width="0" layer="20"/>
<wire x1="54.6" y1="0" x2="54.6" y2="39.0525" width="0" layer="20"/>
<wire x1="54.6" y1="39.0525" x2="0" y2="39.0525" width="0" layer="20"/>
<wire x1="0" y1="39.0525" x2="0" y2="0" width="0" layer="20"/>
<text>Matt Ranostay</text>
<text>Copyright 2016</text>
<text>Hermit Board Rev A6</text>
<text>mranostay@gmail.com</text>
<hole x="2.2225" y="36.83" drill="2.0066"/>
<hole x="52.3875" y="36.83" drill="2.0066"/>
<hole x="2.2225" y="2.2225" drill="2.0066"/>
<hole x="52.3875" y="2.2225" drill="2.0066"/>
</plain>
<libraries>
<library name="mranostay">
<packages>
<package name="ATLAS-OEM">
</package>
<package name="SOT-23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOIC16-1.27-10X3.9MM">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SIP4">
</package>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATLAS_IC" library="mranostay" package="ATLAS-OEM" value="ATLAS-OEM"/>
<element name="U$2" library="mranostay" package="BNC" value="BNCPTH">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MCP1755T" library="mranostay" package="SOT-23-5" value="MCP1755T">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SI8605" library="mranostay" package="SOIC16-1.27-10X3.9MM" value="SI8605">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ROE-0505S" library="mranostay" package="SIP4" value="ROE-0505S"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="R1" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ISO_SDA">
<contactref element="ATLAS_IC" pad="1"/>
<contactref element="SI8605" pad="14"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ISO_SCL">
<contactref element="ATLAS_IC" pad="8"/>
<contactref element="SI8605" pad="11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="ISO_INT">
<contactref element="ATLAS_IC" pad="7"/>
<contactref element="SI8605" pad="12"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="S"/>
<contactref element="ATLAS_IC" pad="4"/>
</signal>
<signal name="PRB_GND">
<contactref element="U$2" pad="GND"/>
<contactref element="ATLAS_IC" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="10"/>
<contactref element="C1" pad="2"/>
<contactref element="ROE-0505S" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SI8605" pad="8"/>
</signal>
<signal name="+5V">
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="ROE-0505S" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="4"/>
<contactref element="SI8605" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="SI8605" pad="6"/>
<contactref element="U$1" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="INT">
<contactref element="SI8605" pad="5"/>
<contactref element="U$1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="+ISO_5V">
<contactref element="MCP1755T" pad="1"/>
<contactref element="MCP1755T" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="ROE-0505S" pad="4"/>
</signal>
<signal name="ISO_GND">
<contactref element="ATLAS_IC" pad="6"/>
<contactref element="MCP1755T" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="MCP1755T" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="ROE-0505S" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="SI8605" pad="9"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="MCP1755T" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="ATLAS_IC" pad="3"/>
<contactref element="SI8605" pad="16"/>
<contactref element="C6" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="SI8605" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
