<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="13.64050625" y2="0" width="0" layer="20"/>
<wire x1="13.64050625" y1="0" x2="13.64050625" y2="32.058009375" width="0" layer="20"/>
<wire x1="13.64050625" y1="32.058009375" x2="0" y2="32.058009375" width="0" layer="20"/>
<wire x1="0" y1="32.058009375" x2="0" y2="0" width="0" layer="20"/>
<text>QFN24</text>
<text>(c)
packom.net
2017</text>
<text>QFN24</text>
<text>*</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Piers's library">
<packages>
<package name="QFN24">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Piers's library" package="QFN24" value="QFN24">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="12"/>
<contactref element="U$1" pad="RI"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="D+"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="9"/>
<contactref element="U$1" pad="D-"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="VIO"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="VDD"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="REGIN"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="VBUS"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="_RST"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="NC"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="GPIO3"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="GPIO2"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="GPIO1"/>
<contactref element="J2" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="GPIO0"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="_SUSPEND"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="VPP"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="SUSPEND"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="CTS"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="RTS"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="RXD"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="TXD"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="DSR"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="DTR"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="DCD"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND1">
<contactref element="J1" pad="11"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="PAD_GND"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
