<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="-4.24" x2="26.67" y2="-4.24" width="0.4064" layer="20"/>
<wire x1="26.67" y1="-4.24" x2="26.67" y2="16.51" width="0.4064" layer="20"/>
<wire x1="26.67" y1="16.51" x2="-1.27" y2="16.51" width="0.4064" layer="20"/>
<wire x1="-1.27" y1="16.51" x2="-1.27" y2="-4.24" width="0.4064" layer="20"/>
<text>IN-</text>
<text>DGND</text>
<text>VS-</text>
<text>A0</text>
<text>A1</text>
<text>WR</text>
<text>OUT</text>
<text>VS+</text>
<text>REF</text>
<text>IN+</text>
<text>AD8253 Instrumentation Amplifier Breakout
Josiah Hester
Clemson University
Rev. A</text>
</plain>
<libraries>
<library name="ad8253">
<packages>
<package name="RM_10">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AD8253" library="ad8253" package="RM_10" value="AD8253ARMZ">
<attribute name="VENDOR" value="Vendor"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AD8253ARMZ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X10" value="M10&quot;">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="IN-">
<contactref element="AD8253" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="DGND">
<contactref element="AD8253" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VS-">
<contactref element="AD8253" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="VS+">
<contactref element="AD8253" pad="8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="IN+">
<contactref element="AD8253" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="WR">
<contactref element="AD8253" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="A0">
<contactref element="AD8253" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="A1">
<contactref element="AD8253" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="REF">
<contactref element="AD8253" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="OUT">
<contactref element="AD8253" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
