<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="-10.795" x2="12.7" y2="-10.795" width="0" layer="20"/>
<wire x1="12.7" y1="-10.795" x2="13.97" y2="-9.525" width="0" layer="20"/>
<wire x1="13.97" y1="-9.525" x2="13.97" y2="9.525" width="0" layer="20"/>
<wire x1="13.97" y1="9.525" x2="12.7" y2="10.795" width="0" layer="20"/>
<wire x1="12.7" y1="10.795" x2="0" y2="10.795" width="0" layer="20"/>
<wire x1="0" y1="10.795" x2="0" y2="-10.795" width="0" layer="20"/>
<hole x="8.255" y="6.35" drill="2.2"/>
<hole x="8.255" y="-6.35" drill="2.2"/>
</plain>
<libraries>
<library name="SAMTEC-BCS-CES-CLx_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 09/08/2012 12:07:08</description>
<packages>
<package name="CUSTOM_16">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SAMTEC-BCS-CES-CLx_By_element14_Batch_1" package="CUSTOM_16" value="CUSTOM_16PAD"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP2" pad="8"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="23"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$7">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$13">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="N$15">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
