<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="25.4" width="0" layer="20"/>
<wire x1="25.4" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>Square Inch Of Power</text>
<text>SHDN</text>
<text>OUTPUT</text>
<text>+</text>
<text>-</text>
<text>GND</text>
</plain>
<libraries>
<library name="PQ_components">
<packages>
<package name="LTC3105DFN">
</package>
<package name="SRU3017-6R8Y">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="0603-CAP">
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="EIA6032">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS">
</package>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="PQ_components" package="LTC3105DFN" value="LTC3105">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="250k">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="787K">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="1.1M">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X01NS" value="In">
<attribute name="VALUE"/>
</element>
<element name="L1" library="PQ_components" package="SRU3017-6R8Y" value="SRU3017-6R8Y">
<attribute name="NAME"/>
</element>
<element name="C32" library="adafruit" package="C0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="33pF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="JP4" library="SparkFun-Connectors" package="1X01NS" value="M01SMDNS"/>
<element name="IC2" library="PQ_components" package="LTC3105DFN" value="LTC3105">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="250k">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="604K">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="1.37M">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
</element>
<element name="L2" library="PQ_components" package="SRU3017-6R8Y" value="SRU3017-6R8Y">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="33pF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="5F supercap">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X02_NO_SILK" value="SHDN"/>
<element name="JP6" library="SparkFun-Connectors" package="1X02_NO_SILK" value="OUTPUT"/>
<element name="C11" library="SparkFun-Capacitors" package="EIA6032" value="470uf"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="P$11"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="P$3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="IC2" pad="P$11"/>
<contactref element="IC2" pad="P$11"/>
<contactref element="R4" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="IC2" pad="P$3"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="C11" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="P$5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="P$1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VIN1">
<contactref element="IC1" pad="P$6"/>
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="JP1" pad="1"/>
<contactref element="C11" pad="P$1"/>
</signal>
<signal name="SHDN">
<contactref element="IC1" pad="P$4"/>
<contactref element="IC2" pad="P$4"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="IC1" pad="P$8"/>
</signal>
<signal name="N$37">
<contactref element="IC1" pad="P$7"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="P$10"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VOUT_MPPT1">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="P$9"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="P$6"/>
<contactref element="IC2" pad="P$6"/>
<contactref element="L2" pad="P$2"/>
<contactref element="C5" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="P$2"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="P$5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="P$1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="P$8"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="P$7"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="P$10"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="P$2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="OUTPUT">
<contactref element="JP6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="P$9"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
