<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20" y2="0" width="0" layer="20"/>
<wire x1="20" y1="0" x2="20" y2="20" width="0" layer="20"/>
<wire x1="20" y1="20" x2="0" y2="20" width="0" layer="20"/>
<wire x1="0" y1="20" x2="0" y2="0" width="0" layer="20"/>
<text>100nF</text>
<text>100nF</text>
<text>10uF</text>
<text>22uF</text>
<text>PWR</text>
<text>DATA</text>
<text>10R</text>
<text>47K</text>
<text>3K3</text>
<text>3K3</text>
<text>VCNL4010</text>
<text>RupTek
VCNL4010 Breakout v1.0
07/16</text>
<text>DATA</text>
<text>PWR</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>GND</text>
<text>3V3</text>
<text>SCL</text>
<text>SDA</text>
<text>INT</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="VCNL4010-GS08">
<packages>
<package name="XDCR_VCNL4010-GS08">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-MINI">
</package>
<package name="GESTURESENSE_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="EIA3216-KIT" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="EIA3216-KIT" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X03" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="DATA">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="3K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="3K3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="VCNL4010-GS08" package="XDCR_VCNL4010-GS08" value="VCNL4010">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-MINI" value=""/>
<element name="U$2" library="SparkFun-Aesthetics" package="GESTURESENSE_NOTEXT" value=""/>
</elements>
<signals>
<signal name="IR_CA">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="C"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="13"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="R3" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="INT">
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="1"/>
<contactref element="C4" pad="A"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="A"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
