<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="18.80949375" x2="0" y2="1.40746875" width="0" layer="20"/>
<wire x1="0" y1="1.40746875" x2="1.40746875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.40746875" y1="0" x2="41.50386875" y2="0" width="0" layer="20"/>
<wire x1="41.50386875" y1="0" x2="43.104" y2="1.60013125" width="0" layer="20" curve="90"/>
<wire x1="43.104" y1="1.60013125" x2="43.104" y2="18.86350625" width="0" layer="20"/>
<wire x1="43.104" y1="18.86350625" x2="41.65750625" y2="20.31" width="0" layer="20" curve="90"/>
<wire x1="41.65750625" y1="20.31" x2="1.50050625" y2="20.31" width="0" layer="20"/>
<wire x1="1.50050625" y1="20.31" x2="0" y2="18.80949375" width="0" layer="20" curve="90"/>
<text>1A Max</text>
<text>12V</text>
<text>GND</text>
<text>GND</text>
<text>12v</text>
<text>LIMIT</text>
<text>RV-Project.Com CC LED Dimmer
</text>
<text>V1.2    4/16/2019</text>
<text>+</text>
<text>+</text>
<text>GND</text>
<text>12V</text>
<text>LIMIT</text>
<text>12v</text>
<text>GND</text>
<text>Power</text>
<text>12V</text>
<text>GND</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="SMD_ELECTROLYTIC_6MMDIA">
</package>
<package name="1206-TANTALUM">
</package>
<package name="SOD-123">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
<package name="1206-RES">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="FUSE476">
</package>
<package name="RV097NS">
</package>
<package name="SMA-DIODE_ALT">
</package>
<package name="1206-CAP">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="a-lib" package="SMD_ELECTROLYTIC_6MMDIA" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="1206-TANTALUM" value="10uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="F931C106KAA "/>
<attribute name="TAYDA" value="A-1822"/>
<attribute name="TYPE" value="Tantalum"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="16V"/>
</element>
<element name="D1" library="a-lib" package="SOD-123" value="TVS-SSOD123">
<attribute name="NAME"/>
</element>
<element name="J1" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="J2" library="a-lib" package="1X03" value="M3HEADER"/>
<element name="R2" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="a-lib" package="SOT223" value="VOLTAGE_REGULATOR_LM117">
<attribute name="NAME"/>
</element>
<element name="F1" library="a-lib" package="FUSE476" value="2.5A">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value="CLIPART_LOGORVPROJECT_XSMALL"/>
<element name="R3" library="a-lib" package="RV097NS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="J2" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="F1" pad="P$2"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="F1" pad="P$1"/>
<contactref element="R3" pad="S1"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="S2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
