<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="85.94" width="0.4064" layer="20"/>
<wire x1="0" y1="85.94" x2="45.81" y2="85.94" width="0.4064" layer="20"/>
<wire x1="45.81" y1="85.94" x2="45.81" y2="0" width="0.4064" layer="20"/>
<wire x1="45.81" y1="0" x2="0" y2="0" width="0.4064" layer="20"/>
<text>OpenROV
Wifi
Top Side
Interface
Board
Rev 0.1</text>
<text>This work is released under the Creative
Commons Attribution-NonCommercial
Share-Alike 3.0 Unported License.
All derivative works are to be attributed
to OpenROV.</text>
<text>Wifi Top Side
Interface Board
Rev 0.1</text>
<text>Battery</text>
<text>+V</text>
<text>GND</text>
</plain>
<libraries>
<library name="OpenROV Topside Interface">
<packages>
<package name="FCI_09-381_2PL">
<description>FCI Terminal Block (2 place)  Series 09-381 Product 20020303</description>
</package>
<package name="SSW-103-02-S-D">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST SOCKET&lt;/b&gt;&lt;p&gt;
Source: Samtec SSW.pdf</description>
</package>
</packages>
</library>
<library name="Walts_Generic_Parts">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="INDUCTOR_3A_TEST">
<description>Test Pads for Generic shielded inductor for ~3A power supplies</description>
</package>
</packages>
</library>
<library name="Walts Generic Connectors">
<packages>
<package name="22-23-2021_ALT_SILK">
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSW-103-02-S-S">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST SOCKET&lt;/b&gt;&lt;p&gt;
Source: Samtec SSW.pdf</description>
</package>
</packages>
</library>
<library name="Walts Power Supply Components">
<packages>
<package name="SO8-THERMAL">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt; SOP-8L&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds31262.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="OpenROV Topside Interface" package="FCI_09-381_2PL" value="FCI 20020303-D021">
<attribute name="NAME"/>
</element>
<element name="J3" library="OpenROV Topside Interface" package="SSW-103-02-S-D" value="SSW-103-01-G-D">
<attribute name="OC_NEWARK" value="11P9365"/>
<attribute name="MPN" value="SSW-103-02-S-D"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="Walts_Generic_Parts" package="R0805" value="1K"/>
<element name="R2" library="Walts_Generic_Parts" package="R0805" value="0 (Jumper)"/>
<element name="J4" library="con-samtec" package="SSW-103-02-S-S" value="SSW-103-02-S-S">
<attribute name="OC_NEWARK" value="11P9367"/>
<attribute name="MPN" value="SSW-103-02-S-S"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="J1" library="Walts Generic Connectors" package="22-23-2021_ALT_SILK" value=""/>
<element name="U1" library="Walts Power Supply Components" package="SO8-THERMAL" value=""/>
<element name="C3" library="Walts_Generic_Parts" package="R0805" value=".1u"/>
<element name="C5" library="Walts_Generic_Parts" package="R0805" value="3.9n"/>
<element name="C4" library="Walts_Generic_Parts" package="R0805" value="10n"/>
<element name="C1" library="Walts_Generic_Parts" package="R1206" value="10u"/>
<element name="C2" library="Walts_Generic_Parts" package="R1206" value="10u"/>
<element name="C6" library="Walts_Generic_Parts" package="R1206" value="22u"/>
<element name="C7" library="Walts_Generic_Parts" package="R1206" value="22u"/>
<element name="R3" library="Walts_Generic_Parts" package="R0805" value="6.8K"/>
<element name="R4" library="Walts_Generic_Parts" package="R0805" value="26.1K"/>
<element name="R5" library="Walts_Generic_Parts" package="R0805" value="10K"/>
<element name="R7" library="Walts_Generic_Parts" package="R0805" value="100K"/>
<element name="L1" library="Walts_Generic_Parts" package="INDUCTOR_3A_TEST" value="10u"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J3" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="J2" pad="1A"/>
<contactref element="J2" pad="1B"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="2B"/>
<contactref element="J2" pad="2A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="PAD"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="R4" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$5">
</signal>
<signal name="N$9">
<contactref element="U1" pad="8"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="6"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="7"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
