<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-11" y1="6" x2="-11" y2="-4" width="0" layer="20"/>
<wire x1="-11" y1="-4" x2="-10" y2="-5" width="0" layer="20" curve="90"/>
<wire x1="-10" y1="-5" x2="9.5857875" y2="-5" width="0" layer="20"/>
<wire x1="9.5857875" y1="-5" x2="11" y2="-3.5857875" width="0" layer="20" curve="90"/>
<wire x1="11" y1="-3.5857875" x2="11" y2="6" width="0" layer="20"/>
<wire x1="11" y1="6" x2="10" y2="7" width="0" layer="20" curve="90"/>
<wire x1="10" y1="7" x2="-10" y2="7" width="0" layer="20"/>
<wire x1="-10" y1="7" x2="-11" y2="6" width="0" layer="20" curve="90"/>
<text>JST-SH-8</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="JST-SH">
<packages>
<package name="JST-SH-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="JST-SH" package="JST-SH-8" value="JST-SH-8"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$8"/>
<contactref element="J1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
