<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="0" y2="24.13" width="0.4064" layer="20"/>
<wire x1="0" y1="24.13" x2="38.1" y2="24.13" width="0.4064" layer="20"/>
<wire x1="38.1" y1="24.13" x2="38.1" y2="1.27" width="0.4064" layer="20"/>
<wire x1="38.1" y1="1.27" x2="0" y2="1.27" width="0.4064" layer="20"/>
<hole x="7.62" y="21.59" drill="2.8"/>
<hole x="7.62" y="3.81" drill="2.8"/>
<text>v2.1</text>
<text>CS</text>
<text>DI</text>
<text>DO</text>
<text>CLK</text>
<text>3.3V</text>
<text>GND</text>
<text>5V</text>
<text>Rugged microSD</text>
</plain>
<libraries>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="Kontakr-custom">
<packages>
<package name="ST1W008S4ER1500">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="40xx" package="SO16" value="4050D"/>
<element name="U$1" library="Kontakr-custom" package="ST1W008S4ER1500" value="ST1W008S4ER1500"/>
<element name="JP1" library="SparkFun-Connectors" package="1X07" value=""/>
<element name="U$2" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="10"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="GND2" route="any" routetag="G$1.GND"/>
<contactref element="U$1" pad="GND3" route="any" routetag="G$1.GND"/>
<contactref element="U$1" pad="GND4" route="any" routetag="G$1.GND"/>
<contactref element="U$1" pad="GND1" route="any" routetag="G$1.GND"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="7"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
