<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="2.54" drill="3.7338"/>
<hole x="48.26" y="2.54" drill="3.7338"/>
<hole x="48.26" y="41.91" drill="3.7338"/>
<hole x="2.54" y="41.91" drill="3.7338"/>
<wire x1="50.8" y1="44.45" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="50.8" y2="44.45" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>5V</text>
<text>12V</text>
<text>10mhz</text>
<text>1mhz</text>
<text>.1</text>
<text>IN</text>
<text>ADJ</text>
<text>OUT</text>
<text>IN</text>
<text>ADJ</text>
<text>OUT</text>
<text>+15</text>
<text>GND</text>
<text>IN</text>
<text>ADJ</text>
<text>OUT</text>
<text>OCXO-REF 1.01 pete@soper.us 9/2014</text>
<text>GND</text>
<text>+12</text>
<text>ADJ</text>
<text>NC</text>
<text>10mhz OUT</text>
<text>CC-BY-SA 3.0</text>
</plain>
<libraries>
<library name="TriEmbed">
<packages>
<package name="TSOP12">
</package>
<package name="OCXO8000">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-ZENER">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SP19L">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="NXP_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:27:46</description>
<packages>
<package name="SOIC127P600X175-16N">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-1.5X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="TriEmbed" package="TSOP12" value="LTC6957-3/4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="10nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="10nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="51">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="pot" package="SP19L" value="5K OSC ADJ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X03" value="7805T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="pot" package="SP19L" value="5K 12V ADJ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03" value="LM317T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X03" value="LM1117T-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X02" value="12V ENBL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-63V" value="1000uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-63V" value="1000uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-DiscreteSemi" package="DIODE-ZENER" value="10V ZENER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="NXP_By_element14_Batch_1" package="SOIC127P600X175-16N" value="74HC390D">
<attribute name="MPN" value="74HC390D"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1085343"/>
<attribute name="OC_NEWARK" value="99K0594"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="3-10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="0-7V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X02" value="PWR LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="TriEmbed" package="OCXO8000" value="OCXO8000"/>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1.5X3" value="FIDUCIAL1.5X3"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1.5X3" value="FIDUCIAL1.5X3"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="12"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="A"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP9" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="S"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="CLK-10M">
<contactref element="IC1" pad="10"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="CLK-1M">
<contactref element="JP8" pad="7"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="E"/>
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="A"/>
<contactref element="R4" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R6" pad="E"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="S"/>
<contactref element="JP4" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="15VDC@2A">
<contactref element="C3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="JP6" pad="3"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP8" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="5"/>
<contactref element="JP5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="+3V3">
<contactref element="JP7" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="JP8" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="11"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="9"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="CLK-100K">
<contactref element="JP8" pad="8"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="JP9" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
