<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="70.79" y2="0" width="0" layer="20"/>
<wire x1="70.79" y1="0" x2="70.79" y2="57.14" width="0" layer="20"/>
<wire x1="70.79" y1="57.14" x2="0" y2="57.14" width="0" layer="20"/>
<wire x1="0" y1="57.14" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUTTON-CONDUCTIVE">
<description>&lt;h3&gt;Conductive Button&lt;/h3&gt;
&lt;p&gt;Used with rubber key pads on the &lt;a href="https://www.sparkfun.com/products/retired/8602"&gt;Nordic Key FOB&lt;/a&gt;. This one was designed and proven to work with the &lt;a href="https://www.sparkfun.com/products/retired/9377"&gt;PolyCase Key FOB enclosures&lt;/a&gt;.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LEFT" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="UP" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="RIGHT" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="DOWN" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="SELECT" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="START" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="B" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="A" library="SparkFun-Switches" package="BUTTON-CONDUCTIVE" value="BUTTON-CONDUCTIVESMD"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="GPIO" library="pinhead" package="1X08" value=""/>
<element name="GND" library="pinhead" package="1X01" value=""/>
<element name="H10" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H11" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H12" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H13" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H15" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
<element name="H16" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="LT">
<contactref element="GPIO" pad="1"/>
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="UP">
<contactref element="GPIO" pad="2"/>
<contactref element="UP" pad="1"/>
</signal>
<signal name="SL">
<contactref element="GPIO" pad="5"/>
<contactref element="SELECT" pad="1"/>
</signal>
<signal name="ST">
<contactref element="GPIO" pad="6"/>
<contactref element="START" pad="1"/>
</signal>
<signal name="B">
<contactref element="GPIO" pad="7"/>
<contactref element="B" pad="1"/>
</signal>
<signal name="A">
<contactref element="GPIO" pad="8"/>
<contactref element="A" pad="1"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="LEFT" pad="2"/>
<contactref element="UP" pad="2"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="DOWN" pad="2"/>
<contactref element="SELECT" pad="2"/>
<contactref element="START" pad="2"/>
<contactref element="B" pad="2"/>
<contactref element="A" pad="2"/>
</signal>
<signal name="DN">
<contactref element="GPIO" pad="3"/>
<contactref element="DOWN" pad="1"/>
</signal>
<signal name="RT">
<contactref element="GPIO" pad="4"/>
<contactref element="RIGHT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
