<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="38.09" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="28.88" y2="0" width="0" layer="20"/>
<wire x1="28.88" y1="0" x2="31.42" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="31.42" y1="2.54" x2="31.42" y2="38.09" width="0" layer="20"/>
<wire x1="31.42" y1="38.09" x2="28.88" y2="40.63" width="0" layer="20" curve="90"/>
<wire x1="28.88" y1="40.63" x2="2.54" y2="40.63" width="0" layer="20"/>
<wire x1="2.54" y1="40.63" x2="0" y2="38.09" width="0" layer="20" curve="90"/>
<text>ATtiny85</text>
<text>ATtiny84</text>
<text>USB</text>
<text>ATtiny84/85 Programmer v3
Created by Michael Backus
tiny.akrobotnerd.com</text>
<text>10uF</text>
</plain>
<libraries>
<library name="Backus">
<packages>
<package name="ARDUINONANO">
</package>
<package name="DIP14">
</package>
<package name="PDIP08_300MIL">
<description>&lt;b&gt;DIL08 300mil&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-5MM-KIT">
<description>2.5 mm spaced PTHs with top copper masked</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Backus" package="ARDUINONANO" value="ARDUINONANO"/>
<element name="U1" library="Backus" package="PDIP08_300MIL" value="ATTINY85-P"/>
<element name="U$2" library="Backus" package="DIP14" value="ATTINY84ATTINY84-20PU"/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM-KIT" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U$2" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$17"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="P$16"/>
</signal>
<signal name="3V3">
<contactref element="U$1" pad="P$29"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$13"/>
<contactref element="U1" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$14"/>
<contactref element="U1" pad="5"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$15"/>
<contactref element="U1" pad="6"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$30"/>
<contactref element="U1" pad="7"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="P$19"/>
<contactref element="U1" pad="8"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="GND2">
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P$3" route="any" routetag="G$1.RST"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="P$18" route="any" routetag="G$1.RST"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
