<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="55.4" y1="37.4" x2="82.8" y2="37.4" width="0" layer="20"/>
<wire x1="82.8" y1="37.4" x2="82.8" y2="64.2" width="0" layer="20"/>
<wire x1="82.8" y1="64.2" x2="55.4" y2="64.2" width="0" layer="20"/>
<wire x1="55.4" y1="64.2" x2="55.4" y2="37.4" width="0" layer="20"/>
<text>Vcc</text>
<text>GND</text>
<text>SCLK</text>
<text>MOSI</text>
<text>MISO</text>
<text>!EOC</text>
<text>A0</text>
<text>1</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>!CS</text>
<text>AVDD</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>T. Kircher</text>
<text>8 channel 16-bit ADC</text>
<text>IC1</text>
<text>MAX1168</text>
<text>A4</text>
<text>2</text>
<text>3</text>
</plain>
<libraries>
<library name="thomas">
<description>Dr. K's collection of Eagle CAD footprints for projects</description>
<packages>
<package name="QSOP-24">
<description>This is a quarter-size (QSOP-28) footprint, from Maxim IC.</description>
</package>
<package name="0805">
<description>This 0805 (2012 metric) footprint has 1.0mm x 1.2mm pads, with a 1.2mm gap. Specification from Panasonic. Verified 8/15/2011</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="thomas" package="QSOP-24" value="MAX1168"/>
<element name="C1" library="thomas" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="thomas" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="thomas" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="thomas" package="0805" value="10">
<attribute name="NAME"/>
</element>
<element name="C4" library="thomas" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J14" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J15" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="U$9" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="SJ1" library="jumper" package="SJ_2" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SCLK">
<contactref element="IC1" pad="P4"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="P3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="ENABLE">
<contactref element="IC1" pad="P20"/>
<contactref element="J15" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="P17"/>
<contactref element="IC1" pad="P18"/>
<contactref element="IC1" pad="P21"/>
<contactref element="J14" pad="1"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="P15"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="P16"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="P19"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="ANALOG6">
<contactref element="IC1" pad="P13"/>
<contactref element="J11" pad="1"/>
</signal>
<signal name="ANALOG7">
<contactref element="IC1" pad="P14"/>
<contactref element="J12" pad="1"/>
</signal>
<signal name="ANALOG0">
<contactref element="IC1" pad="P7"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="ANALOG1">
<contactref element="IC1" pad="P8"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="ANALOG2">
<contactref element="IC1" pad="P9"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="ANALOG3">
<contactref element="IC1" pad="P10"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="ANALOG4">
<contactref element="IC1" pad="P11"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="ANALOG5">
<contactref element="IC1" pad="P12"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="P22"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="P1"/>
<contactref element="J13" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="P5"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="!EOC">
<contactref element="IC1" pad="P6"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="P2"/>
<contactref element="SJ1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
