<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.27" x2="0" y2="15.59" width="0.3048" layer="20"/>
<wire x1="2.27" y1="17.86" x2="88.73" y2="17.86" width="0.3048" layer="20"/>
<wire x1="88.73" y1="17.86" x2="91" y2="15.59" width="0.3048" layer="20" curve="-90"/>
<wire x1="91" y1="15.59" x2="91" y2="2.27" width="0.3048" layer="20"/>
<text>D:/SmartProjects/Snc/a4_bn_logo2.bmp</text>
<wire x1="2.27" y1="0" x2="88.73" y2="0" width="0.3048" layer="20"/>
<wire x1="91" y1="2.27" x2="88.73" y2="0" width="0.3048" layer="20" curve="-90"/>
<wire x1="2.27" y1="0" x2="0" y2="2.27" width="0.3048" layer="20" curve="-90"/>
<hole x="2.54" y="15.32" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<hole x="88.55" y="15.32" drill="3.2"/>
<hole x="88.55" y="2.54" drill="3.2"/>
<wire x1="0" y1="15.59" x2="2.27" y2="17.86" width="0.3048" layer="20" curve="-90"/>
<text>Charging
Dock 2.1</text>
<text>5V 2.5A supply
Six 400mAh batteries</text>
<text>Charging
Dock 2.1</text>
</plain>
<libraries>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Andy-library">
<packages>
<package name="BARREL_CONN">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="Cerebro-library">
<packages>
<package name="MICRO_LOCK_2PIN">
</package>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Andy-library" package="BARREL_CONN" value="POWER_JACK&quot;">
<attribute name="DIGIKEY_PN" value="CP-037A-ND"/>
<attribute name="MANUFACTURER" value="CUI Inc"/>
<attribute name="MFG_PN" value="PJ-037A"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R3" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED1" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN1" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R5" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C3" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R7" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED3" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN3" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R9" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN3" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C5" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R13" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED5" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN5" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R14" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R15" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN5" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C9" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R19" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED7" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN7" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R20" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R21" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN7" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C13" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R25" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED9" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN9" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R26" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R27" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN9" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C17" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="R31" library="Andy-library" package="0805" value="2.5k">
<attribute name="VALUE"/>
</element>
<element name="RED11" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="GREEN11" library="Andy-library" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R32" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="R33" library="Cerebro-library" package="0805" value="470">
<attribute name="VALUE"/>
</element>
<element name="CN11" library="Cerebro-library" package="MICRO_LOCK_2PIN" value=""/>
<element name="C21" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="Cerebro-library" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="GND"/>
<contactref element="U5" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="GREEN5" pad="K"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="CN5" pad="P$1"/>
<contactref element="U7" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="GREEN7" pad="K"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="CN7" pad="P$1"/>
<contactref element="U11" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="GREEN11" pad="K"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="CN11" pad="P$1"/>
<contactref element="U3" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="GREEN3" pad="K"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="CN3" pad="P$1"/>
<contactref element="U1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="GREEN1" pad="K"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="CN1" pad="P$1"/>
<contactref element="U9" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="GREEN9" pad="K"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="CN9" pad="P$1"/>
</signal>
<signal name="5VDC">
<contactref element="J1" pad="PWR"/>
<contactref element="U1" pad="4"/>
<contactref element="RED1" pad="A"/>
<contactref element="C3" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="RED3" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="RED5" pad="A"/>
<contactref element="C9" pad="1"/>
<contactref element="U7" pad="4"/>
<contactref element="RED7" pad="A"/>
<contactref element="C13" pad="1"/>
<contactref element="U9" pad="4"/>
<contactref element="RED9" pad="A"/>
<contactref element="C17" pad="1"/>
<contactref element="U11" pad="4"/>
<contactref element="RED11" pad="A"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="NW_CHARGE1">
<contactref element="U1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="CN1" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="RED1" pad="K"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="2"/>
<contactref element="GREEN1" pad="A"/>
</signal>
<signal name="NW_CHARGE3">
<contactref element="U3" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="CN3" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="5"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="RED3" pad="K"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R8" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="2"/>
<contactref element="GREEN3" pad="A"/>
</signal>
<signal name="NW_CHARGE5">
<contactref element="U5" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="CN5" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="U5" pad="5"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="RED5" pad="K"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R14" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R15" pad="2"/>
<contactref element="GREEN5" pad="A"/>
</signal>
<signal name="NW_CHARGE7">
<contactref element="U7" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="CN7" pad="P$2"/>
</signal>
<signal name="N$26">
<contactref element="U7" pad="5"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="RED7" pad="K"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R20" pad="2"/>
<contactref element="U7" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R21" pad="2"/>
<contactref element="GREEN7" pad="A"/>
</signal>
<signal name="NW_CHARGE9">
<contactref element="U9" pad="3"/>
<contactref element="C18" pad="1"/>
<contactref element="CN9" pad="P$2"/>
</signal>
<signal name="N$34">
<contactref element="U9" pad="5"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="RED9" pad="K"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R26" pad="2"/>
<contactref element="U9" pad="1"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R27" pad="2"/>
<contactref element="GREEN9" pad="A"/>
</signal>
<signal name="NW_CHARGE11">
<contactref element="U11" pad="3"/>
<contactref element="C22" pad="1"/>
<contactref element="CN11" pad="P$2"/>
</signal>
<signal name="N$42">
<contactref element="U11" pad="5"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="RED11" pad="K"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="R32" pad="2"/>
<contactref element="U11" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R33" pad="2"/>
<contactref element="GREEN11" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
