<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.24" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="0" x2="15.24" y2="17.78" width="0" layer="20"/>
<wire x1="15.24" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>A</text>
<text>B</text>
<text>COM</text>
<text>S1</text>
<text>S2</text>
<text>14OCT2013</text>
<text>C.SCHNAREL</text>
<text>EN12-VS</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
<library name="ChipsParts">
<packages>
<package name="EN12-VS">
<description>Switch, rotary encoder, gray code + push button (NO), TT Electronics, EN12-VS, from TT Electronics datasheet 05/13/08.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="ChipsParts" package="EN12-VS" value="ROTARY_ENCODER-EN12-VS"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="4"/>
<contactref element="S1" pad="D"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="5"/>
<contactref element="S1" pad="E"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="3"/>
<contactref element="S1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="2"/>
<contactref element="S1" pad="COM"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="1"/>
<contactref element="S1" pad="B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
