<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="24.13" y1="0" x2="26.3525" y2="2.2225" width="0" layer="20" curve="90"/>
<wire x1="26.3525" y1="2.2225" x2="26.3525" y2="15.5575" width="0" layer="20"/>
<wire x1="26.3525" y1="15.5575" x2="24.13" y2="17.78" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="17.78" x2="2.54" y2="17.78" width="0" layer="20"/>
<wire x1="2.54" y1="17.78" x2="0" y2="15.24" width="0" layer="20" curve="90"/>
<wire x1="0" y1="15.24" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5*</text>
<text>6*</text>
<text>7*</text>
<text>RST</text>
<text>8*</text>
<text>9</text>
<text>10</text>
<text>GND</text>
<text>VCC</text>
<text>ATtiny84</text>
<text>Barbary</text>
<text>Enterprises</text>
<text>Barbary</text>
<text>Enterprises</text>
<text>Pixie</text>
<text>84</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL14">
</package>
</packages>
</library>
<library name="barbary_enterprises">
<packages>
<package name="2X3">
</package>
<package name="M8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TINY" library="SparkFun-DigitalIC" package="DIL14" value="ATTINY84ATTINY84-20PU"/>
<element name="ICSP" library="barbary_enterprises" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="U$1" library="barbary_enterprises" package="M8" value="M8"/>
<element name="U$2" library="barbary_enterprises" package="M8" value="M8"/>
</elements>
<signals>
<signal name="GND">
<contactref element="TINY" pad="14"/>
<contactref element="ICSP" pad="6"/>
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="TINY" pad="1"/>
<contactref element="ICSP" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="TINY" pad="4"/>
<contactref element="ICSP" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="D5">
<contactref element="TINY" pad="8"/>
<contactref element="ICSP" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="D6">
<contactref element="TINY" pad="7"/>
<contactref element="ICSP" pad="4"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="D4">
<contactref element="TINY" pad="9"/>
<contactref element="ICSP" pad="3"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="D0">
<contactref element="TINY" pad="13"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="D1">
<contactref element="TINY" pad="12"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="D2">
<contactref element="TINY" pad="11"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="D3">
<contactref element="TINY" pad="10"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="D7">
<contactref element="TINY" pad="6"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="D8">
<contactref element="TINY" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="D9">
<contactref element="TINY" pad="3"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="D10">
<contactref element="TINY" pad="5"/>
<contactref element="U$1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
