<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.635" x2="38.1" y2="-0.635" width="0" layer="20"/>
<wire x1="38.1" y1="-0.635" x2="38.1" y2="42.545" width="0" layer="20"/>
<wire x1="38.1" y1="42.545" x2="0" y2="42.545" width="0" layer="20"/>
<wire x1="0" y1="42.545" x2="0" y2="-0.635" width="0" layer="20"/>
<text>Cohesion3D Micro Smoothie Brain</text>
<text>2.54mm Header Breakout Board</text>
<text>EN1</text>
<text>DIR1</text>
<text>STP1</text>
<text>EN2</text>
<text>DIR2</text>
<text>STP2</text>
<text>EN3</text>
<text>DIR3</text>
<text>STP3</text>
<text>EN4</text>
<text>DIR4</text>
<text>STP4</text>
<text>EN5</text>
<text>DIR5</text>
<text>STP5</text>
<text>P2.7</text>
<text>P2.6</text>
<text>P2.5</text>
<text>P2.4</text>
<text>P1.23</text>
<text>P1.22</text>
<text>P0.16</text>
<text>P0.15</text>
<text>P0.18</text>
<text>P3.25</text>
<text>P3.26</text>
<text>P1.30</text>
<text>Tx</text>
<text>Rx</text>
<text>X-MN</text>
<text>X-MX</text>
<text>Y-MN</text>
<text>Y-MX</text>
<text>Z-MN</text>
<text>Z-MX</text>
<text>Gnd</text>
<text>5vin</text>
<text>3.3v</text>
<text>TH4</text>
<text>TH3</text>
<text>TH2</text>
<text>TH1</text>
<text>AVCC</text>
<text>AGnd</text>
<text>Cohesion3D Micro Smoothie Brain</text>
<text>2.54mm Header Breakout Board</text>
<text>Designed by Ray Kholodovsky</text>
</plain>
<libraries>
<library name="Micro-Smoothie-Brain">
<packages>
<package name="SMOOTHIE-STAMP-PTH">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
</package>
<package name="1X14">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Micro-Smoothie-Brain" package="SMOOTHIE-STAMP-PTH" value="SMOOTHIE-STAMPSMOOTHIE-STAMP-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X14" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="EN1"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="14"/>
<contactref element="U$1" pad="DIR1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="13"/>
<contactref element="U$1" pad="STP1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="EN2"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="11"/>
<contactref element="U$1" pad="DIR2"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="10"/>
<contactref element="U$1" pad="STP2"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="9"/>
<contactref element="U$1" pad="EN3"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="DIR3"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="STP3"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="EN4"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="DIR4"/>
</signal>
<signal name="N$13">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="STP4"/>
</signal>
<signal name="N$14">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="EN5"/>
</signal>
<signal name="N$15">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="DIR5"/>
</signal>
<signal name="N$16">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="STP5"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="P2.7_HOTEND_FET"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="PWM1_BED_HEATER"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="P2.6_FAN_FET"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="PWM0_PSU_OUT"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="P1_22-3RD-SMALL-FET"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="P1_23-3RD-LARGE-FET"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="SCK1"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="SSEL1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="MOSI1"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="P1_30_CLICK-ON-RRD"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="SD_IRQ-ENC-A-ON-RRD"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="SD_WP-ENC-B-ON-RRD"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V"/>
<contactref element="JP3" pad="14"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="3.3V"/>
<contactref element="JP3" pad="13"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="JP3" pad="15"/>
</signal>
<signal name="RX_0">
<contactref element="U$1" pad="RX_0"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="TX_0">
<contactref element="U$1" pad="TX_0"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="X_MIN"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="U$1" pad="X_MAX"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="U$1" pad="Y_MIN"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="Y_MAX"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$35">
<contactref element="U$1" pad="Z_MIN"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$36">
<contactref element="U$1" pad="Z_MAX"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$37">
<contactref element="U$1" pad="AVCC"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="TH1_HOTEND"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="N$39">
<contactref element="U$1" pad="TH2_BED"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="N$40">
<contactref element="U$1" pad="TH3"/>
<contactref element="JP3" pad="11"/>
</signal>
<signal name="N$41">
<contactref element="U$1" pad="TH4"/>
<contactref element="JP3" pad="12"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="AGND"/>
<contactref element="JP3" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
