<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<board>
<plain>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>GREEN</text>
<text>YELLOW</text>
<text>VOUT</text>
<text>REG</text>
<wire x1="30.861" y1="38.989" x2="34.3662" y2="35.4838" width="0.254" layer="20"/>
<wire x1="34.3662" y1="35.4838" x2="34.3662" y2="1.6002" width="0.254" layer="20"/>
<wire x1="34.3662" y1="1.6002" x2="34.1376" y2="1.3716" width="0.254" layer="20"/>
<wire x1="34.1376" y1="1.3716" x2="31.0134" y2="-1.7526" width="0.254" layer="20"/>
<wire x1="31.0134" y1="-1.7526" x2="30.6578" y2="-1.7526" width="0.254" layer="20"/>
<wire x1="30.6578" y1="-1.7526" x2="4.4958" y2="-1.7526" width="0.254" layer="20"/>
<wire x1="4.4958" y1="-1.7526" x2="0.8636" y2="1.8796" width="0.254" layer="20"/>
<wire x1="0.8636" y1="1.9812" x2="0.8636" y2="35.5092" width="0.254" layer="20"/>
<wire x1="0.8636" y1="35.5092" x2="4.318" y2="38.9636" width="0.254" layer="20"/>
<wire x1="4.318" y1="38.9636" x2="4.3434" y2="38.989" width="0.254" layer="20"/>
<wire x1="4.318" y1="38.9636" x2="30.861" y2="38.9636" width="0.254" layer="20"/>
<wire x1="30.861" y1="38.9636" x2="30.8864" y2="38.989" width="0.254" layer="20"/>
<text>VBAT</text>
<text>GND</text>
<text>RX3</text>
<text>TX3</text>
<text>TX1</text>
<text>TX1</text>
</plain>
<libraries>
<library name="headers(2mm)">
<packages>
<package name="1X4">
</package>
<package name="1X10">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="headers(2mm)" package="1X4" value="1X4"/>
<element name="U$1" library="headers(2mm)" package="1X10" value="1X10"/>
<element name="U$3" library="headers(2mm)" package="1X10" value="1X10"/>
<element name="J1" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD9" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD10" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD11" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD12" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD13" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD14" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD15" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD16" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD17" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD18" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="REG" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="10"/>
<contactref element="J2" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="REG" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="U$3" pad="9"/>
<contactref element="REG" pad="3"/>
</signal>
<signal name="5V">
<contactref element="U$2" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="REG" pad="1"/>
</signal>
<signal name="MRX_STX">
<contactref element="U$2" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MTX_SRX">
<contactref element="U$2" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="TX1">
<contactref element="J4" pad="3"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
