<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.4" y1="42.08" x2="0.4" y2="5.3050125" width="0" layer="20"/>
<wire x1="0.4" y1="5.3050125" x2="5.6637625" y2="0.04125" width="0" layer="20" curve="90"/>
<wire x1="5.6637625" y1="0.04125" x2="6.232075" y2="0.04125" width="0" layer="20"/>
<wire x1="6.232075" y1="0.04125" x2="11.63" y2="5.439175" width="0" layer="20" curve="90"/>
<wire x1="11.63" y1="5.439175" x2="11.6" y2="38.8" width="0" layer="20"/>
<wire x1="11.6" y1="38.8" x2="11.6" y2="42.08" width="0" layer="20"/>
<wire x1="11.6" y1="42.08" x2="0.4" y2="42.08" width="0" layer="20"/>
<hole x="6" y="34" drill="3.2"/>
<hole x="6" y="20" drill="3.2"/>
</plain>
<libraries>
<library name="SJR_thonkiconn">
<packages>
<package name="THONKICONN">
</package>
</packages>
</library>
<library name="TomW">
<packages>
<package name="D6_BUTTON_RND">
<description>Momentary Pushbutton Switch</description>
</package>
</packages>
</library>
<library name="MB2015_resistors">
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="mb_supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="OCTOGON">
<description>&lt;b&gt;Octogonal Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN" library="SJR_thonkiconn" package="THONKICONN" value="THONKICONN"/>
<element name="OUT" library="SJR_thonkiconn" package="THONKICONN" value="THONKICONN"/>
<element name="SWITCH" library="TomW" package="D6_BUTTON_RND" value="D6_PUSH_SWITCH"/>
<element name="R1" library="MB2015_resistors" package="R0207/3" value="100K"/>
<element name="SW" library="mb_supply" package="OCTOGON" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IN" pad="P$1"/>
<contactref element="OUT" pad="P$1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="OUT" pad="P$3"/>
<contactref element="SWITCH" pad="P$1"/>
<contactref element="SWITCH" pad="P$2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IN" pad="P$3"/>
<contactref element="SWITCH" pad="P$3"/>
<contactref element="SWITCH" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="IN" pad="P$2"/>
<contactref element="SW" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
