<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="19.05" y2="13.335" width="0" layer="20"/>
<wire x1="19.05" y1="13.335" x2="0" y2="13.335" width="0" layer="20"/>
<wire x1="0" y1="13.335" x2="0" y2="0" width="0" layer="20"/>
<text>TR1</text>
<text>TR2</text>
<text>COR3D Mini PWR K40</text>
<text>Gnd</text>
<text>24v</text>
<text>PWM</text>
<text>5v</text>
<text>COR3D Mini PWR K40</text>
<text>LO</text>
<text>5v</text>
<text>Gnd</text>
<text>24v</text>
<text>5v-L</text>
<text>Designed by Ray Kholodovsky</text>
<text>24v</text>
<text>Gnd</text>
<text>5v</text>
<text>LO</text>
<text>COR3D Mini PWR K40</text>
<text>5v</text>
<text>PWM</text>
<text>Gnd</text>
<text>24v</text>
<text>Gnd</text>
<text>Gnd</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP13" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP14" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="JP13" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="SJ1" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="24V">
<contactref element="JP13" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP14" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP14" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="LO">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="PWM">
<contactref element="JP13" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5V-LASER">
<contactref element="SJ1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
