<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="38.1" width="0.1524" layer="20"/>
<wire x1="0" y1="38.1" x2="203.2" y2="38.1" width="0.1524" layer="20"/>
<wire x1="203.2" y1="38.1" x2="203.2" y2="0" width="0.1524" layer="20"/>
<wire x1="203.2" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
<hole x="6.35" y="6.35" drill="5.1054"/>
<hole x="6.35" y="31.75" drill="5.1054"/>
<hole x="44.45" y="6.35" drill="5.1054"/>
<hole x="44.45" y="31.75" drill="5.1054"/>
<hole x="82.55" y="6.35" drill="5.1054"/>
<hole x="82.55" y="31.75" drill="5.1054"/>
<hole x="120.65" y="6.35" drill="5.1054"/>
<hole x="120.65" y="31.75" drill="5.1054"/>
<hole x="158.75" y="6.35" drill="5.1054"/>
<hole x="158.75" y="31.75" drill="5.1054"/>
<hole x="196.85" y="6.35" drill="5.1054"/>
<hole x="196.85" y="31.75" drill="5.1054"/>
<text>Power Distribution Board, 5V
Torch Technologies, Inc.
Rev. B      02/06/2018.</text>
<text>Power Distribution Board, 5V.
Torch Technologies, Inc.
Rev. B      02/06/2018.</text>
</plain>
<libraries>
<library name="astro_work">
<packages>
<package name="5-103669-1">
</package>
<package name="MOLEX-MINI-FIT-4">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="astro">
<packages>
<package name="TORCH_LOGO3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="PANASONIC_C" value="22uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08618"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="PANASONIC_C" value="22uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08618"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="astro" package="TORCH_LOGO3" value=""/>
<element name="U$2" library="astro" package="TORCH_LOGO3" value=""/>
<element name="J1" library="astro_work" package="5-103669-1" value="A33893-ND"/>
<element name="J2" library="astro_work" package="5-103669-1" value="A33893-ND"/>
<element name="J3" library="astro_work" package="5-103669-1" value="A33893-ND"/>
<element name="J4" library="astro_work" package="5-103669-1" value="A33893-ND"/>
<element name="X1" library="astro_work" package="MOLEX-MINI-FIT-4" value="MOLEX-MINI-FIT-4"/>
<element name="X2" library="astro_work" package="MOLEX-MINI-FIT-4" value="MOLEX-MINI-FIT-4"/>
<element name="X3" library="astro_work" package="MOLEX-MINI-FIT-4" value="MOLEX-MINI-FIT-4"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="3"/>
<contactref element="X2" pad="1"/>
<contactref element="X2" pad="3"/>
<contactref element="X3" pad="1"/>
<contactref element="X3" pad="3"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="2"/>
<contactref element="X3" pad="4"/>
<contactref element="X3" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="+"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
