<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="18.88125" x2="0" y2="7.184203125" width="0" layer="20"/>
<wire x1="0" y1="7.184203125" x2="7.184203125" y2="0" width="0" layer="20"/>
<wire x1="7.184203125" y1="0" x2="23.295796875" y2="0" width="0" layer="20"/>
<wire x1="23.295796875" y1="0" x2="30.48" y2="7.184203125" width="0" layer="20"/>
<wire x1="30.48" y1="7.184203125" x2="30.48" y2="18.88125" width="0" layer="20"/>
<wire x1="30.48" y1="18.88125" x2="0" y2="18.88125" width="0" layer="20"/>
<text>INB</text>
<text>INJ</text>
<text>GND</text>
<text>OUTJ</text>
<text>OUTB</text>
<text>LED+</text>
<text>LED+</text>
<text>KO Amps 3PDT
v1.2 2021</text>
<text>+</text>
<text>+</text>
</plain>
<libraries>
<library name="diodes">
<packages>
<package name="3MM_D">
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="GROUND">
<description>Square shaped GROUND pad</description>
</package>
<package name="OCTO">
<description>Octogon shaped IN pad</description>
</package>
<package name="UNLABELED">
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="3PDT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diodes" package="3MM_D" value="LED"/>
<element name="GND" library="supply pins" package="GROUND" value="SQUAREPAD"/>
<element name="INJ" library="supply pins" package="OCTO" value="OCTOPAD"/>
<element name="OUTB" library="supply pins" package="OCTO" value="OCTOPAD"/>
<element name="SW1" library="switches" package="3PDT" value="3PDT"/>
<element name="INB" library="supply pins" package="OCTO" value="OCTOPAD"/>
<element name="U$3" library="supply pins" package="UNLABELED" value="ROUNDPAD"/>
<element name="U$5" library="supply pins" package="OCTO" value="OCTOPAD"/>
<element name="D2" library="diodes" package="3MM_D" value="LED"/>
<element name="U$1" library="supply pins" package="UNLABELED" value="ROUNDPAD"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SW1" pad="B2"/>
<contactref element="GND" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="B1"/>
<contactref element="D1" pad="P$1"/>
<contactref element="D2" pad="P$1"/>
</signal>
<signal name="LED">
<contactref element="D1" pad="ANODE"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="SW1" pad="B3"/>
<contactref element="SW1" pad="C3"/>
</signal>
<signal name="INJ">
<contactref element="INJ" pad="P$1"/>
<contactref element="SW1" pad="C1"/>
<contactref element="SW1" pad="A3"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="ANODE"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="OUTJ">
<contactref element="U$5" pad="P$1"/>
<contactref element="SW1" pad="A2"/>
</signal>
<signal name="INB">
<contactref element="INB" pad="P$1"/>
<contactref element="SW1" pad="C2"/>
</signal>
<signal name="OUTB">
<contactref element="SW1" pad="A1"/>
<contactref element="OUTB" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
