<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0.2032" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="20.32" width="0.2032" layer="20"/>
<wire x1="35.56" y1="20.32" x2="0" y2="20.32" width="0.2032" layer="20"/>
<wire x1="0" y1="20.32" x2="0" y2="0" width="0.2032" layer="20"/>
<text>VCC</text>
<text>VINL</text>
<text>VINR</text>
<text>MD1</text>
<text>MD0</text>
<text>FMT1</text>
<text>FMT0</text>
<text>GND</text>
<text>LRCK</text>
<text>BCK</text>
<text>DOUT</text>
<text>PDWN</text>
<text>PCM1803 Breakout alonper</text>
<text>7-2-18</text>
<text>3.3V</text>
<text>BPAS</text>
<text>MSCK</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="EIA3216">
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun" package="SOT23-5" value="5V_REG"/>
<element name="U2" library="SparkFun" package="SOT23-5" value="3.3V_REG"/>
<element name="C1" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C2" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C5" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C6" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C7" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C8" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="U3" library="SparkFun" package="SSOP20" value="PCM1803SMD"/>
<element name="C11" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C12" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C14" library="SparkFun" package="0402-CAP" value="0.1uF"/>
<element name="SJ3" library="SparkFun" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE"/>
<element name="JP3" library="SparkFun" package="1X08" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X07" value=""/>
</elements>
<signals>
<signal name="5V">
<contactref element="U1" pad="5"/>
<contactref element="U3" pad="5"/>
<contactref element="C5" pad="A"/>
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="14"/>
<contactref element="C6" pad="A"/>
<contactref element="C8" pad="1"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="DGND">
<contactref element="U3" pad="13"/>
<contactref element="U3" pad="9"/>
<contactref element="U2" pad="2"/>
<contactref element="C6" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="4"/>
<contactref element="C11" pad="A"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U3" pad="3"/>
<contactref element="C13" pad="A"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="MD1">
<contactref element="U3" pad="20"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="MD0">
<contactref element="U3" pad="19"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="FMT1">
<contactref element="U3" pad="18"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="FMT0">
<contactref element="U3" pad="17"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="VINL">
<contactref element="U3" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VINR">
<contactref element="U3" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="BPAS">
<contactref element="U3" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="PDWN">
<contactref element="U3" pad="7"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="DOUT">
<contactref element="U3" pad="12"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="BCK">
<contactref element="U3" pad="11"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="LRCK">
<contactref element="U3" pad="10"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C11" pad="C"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="C"/>
<contactref element="C14" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="C"/>
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="6"/>
<contactref element="SJ3" pad="1"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MSCK">
<contactref element="U3" pad="15"/>
<contactref element="JP2" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
