<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0.005" y1="22.68180625" x2="0.005" y2="0.81319375" width="0.254" layer="20"/>
<wire x1="0.005" y1="0.81319375" x2="0.65319375" y2="0.165" width="0.254" layer="20" curve="90"/>
<wire x1="0.65319375" y1="0.165" x2="34.90680625" y2="0.165" width="0.254" layer="20"/>
<wire x1="34.90680625" y1="0.165" x2="35.555" y2="0.81319375" width="0.254" layer="20" curve="90"/>
<wire x1="35.555" y1="0.81319375" x2="35.555" y2="22.672084375" width="0.254" layer="20"/>
<wire x1="35.555" y1="22.672084375" x2="34.897084375" y2="23.33" width="0.254" layer="20" curve="90"/>
<wire x1="34.897084375" y1="23.33" x2="0.65319375" y2="23.33" width="0.254" layer="20"/>
<wire x1="0.65319375" y1="23.33" x2="0.005" y2="22.68180625" width="0.254" layer="20" curve="90"/>
<text>+++</text>
<text>GND</text>
<text>MISO</text>
<text>SCK</text>
<text>MOSI</text>
<text>RST</text>
<text>GND</text>
<text>+5V</text>
<text>---</text>
<text>---</text>
<text>+++</text>
<text>+++</text>
<text>GDS</text>
<text>GDS</text>
<text>(C)2022 GLM Tiny1</text>
<text>Max VDC - Check C2
Double Check Polarity
Omit C1 if Q1 populated</text>
</plain>
<libraries>
<library name="zetex-zxld1360">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
</packages>
</library>
<library name="diode-special-packages">
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="inductor-power">
<packages>
<package name="DR12X">
<description>Layout for Coiltronics DR125 and 127&lt;BR&gt;
12mm sq. inductors</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AVR_MINI_PROG">
</package>
</packages>
</library>
<library name="transistor-generic">
<description>&lt;B&gt;Generic Transistors&lt;/B&gt;&lt;P&gt;

Just some plain vanilla GP transistors, in various packages.</description>
<packages>
<package name="TO251AA-V">
<description>&lt;b&gt;I-Pak&lt;/b&gt; International Rectifier</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="zetex-zxld1360" package="SOT23-5L" value="ZXLD1360">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode-special-packages" package="SOD123" value="35V">
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="R1210" value="R560">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C1210" value="4.7u 35v">
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C1206" value="1u 20v"/>
<element name="L1" library="inductor-power" package="DR12X" value="68uh DR12X"/>
<element name="BAT" library="rcl" package="R2512" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603K" value="10n (optional)">
<attribute name="NAME"/>
</element>
<element name="IC2" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="SparkFun-PowerIC" package="SOT23-5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="100n">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="AVR_MINI_PROG" value=""/>
<element name="R2" library="rcl" package="R0603" value="100R">
<attribute name="NAME"/>
</element>
<element name="Q2" library="transistor-generic" package="TO251AA-V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-generic" package="TO251AA-V" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="rcl" package="R2512" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="rcl" package="R2512" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="100R">
<attribute name="NAME"/>
</element>
<element name="R4" library="rcl" package="R0603" value="100R">
<attribute name="NAME"/>
</element>
<element name="D2" library="diode-special-packages" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="diode-special-packages" package="SOD123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="4K7">
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0603" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+12V">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="D1" pad="K"/>
<contactref element="C2" pad="1"/>
<contactref element="BAT" pad="2"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="BAT" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="ICSP" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="LX">
<contactref element="IC1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="P$2"/>
</signal>
<signal name="ISNS">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="LED-">
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="ADJ">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ADJCTL">
<contactref element="R2" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="DRAINLED1">
<contactref element="Q2" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="DRAINLED2">
<contactref element="Q3" pad="2"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="GATEQ2">
<contactref element="D3" pad="A"/>
<contactref element="Q2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="GATEQ3">
<contactref element="D2" pad="A"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="CTLED1">
<contactref element="R4" pad="2"/>
<contactref element="D3" pad="K"/>
<contactref element="ICSP" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="CTLED2">
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="K"/>
<contactref element="ICSP" pad="3"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="7"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="6"/>
<contactref element="ICSP" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
