<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="32.3" y1="13.4" x2="-0.003" y2="13.4" width="0" layer="20"/>
<wire x1="-0.003" y1="13.4" x2="-0.003" y2="-0.005" width="0" layer="20"/>
<wire x1="-0.003" y1="-0.005" x2="32.3" y2="-0.005" width="0" layer="20"/>
<wire x1="32.3" y1="-0.005" x2="32.3" y2="13.4" width="0" layer="20"/>
<text>17</text>
<text>CC1101 868MS10
RPi SPI Adaptor V0.3</text>
<text>CC-BY-SA
codm.de</text>
<text>GDO0=GPIO25
GDO2=GPIO24</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="codm">
<packages>
<package name="CC1101-868MS10">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="U.FL">
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X05" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="codm" package="CC1101-868MS10" value="CC1101-868MS10"/>
<element name="X1" library="adafruit" package="U.FL" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="VCC"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="MOSI"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="MISO"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="GDO2">
<contactref element="U$1" pad="GDO2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="SCK"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="CSN">
<contactref element="U$1" pad="CSN"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="ANT">
<contactref element="U$1" pad="ANT"/>
<contactref element="JP2" pad="1"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND@0"/>
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="GDO0">
<contactref element="U$1" pad="GDO0"/>
<contactref element="JP1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
