<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<hole x="12.4206" y="57.4294" drill="3.2"/>
<hole x="57.4294" y="57.4294" drill="3.2"/>
<hole x="12.4206" y="12.4206" drill="3.2"/>
<hole x="57.4294" y="12.4206" drill="3.2"/>
<wire x1="0" y1="58.42" x2="0" y2="11.43" width="0" layer="20"/>
<wire x1="11.43" y1="0" x2="58.42" y2="0" width="0" layer="20"/>
<wire x1="69.85" y1="11.43" x2="69.85" y2="58.42" width="0" layer="20"/>
<wire x1="58.42" y1="69.85" x2="37.465" y2="69.85" width="0" layer="20"/>
<wire x1="20.955" y1="69.85" x2="11.43" y2="69.85" width="0" layer="20"/>
<wire x1="20.955" y1="69.85" x2="20.955" y2="55.245" width="0" layer="20"/>
<wire x1="20.955" y1="55.245" x2="37.465" y2="55.245" width="0" layer="20"/>
<wire x1="37.465" y1="55.245" x2="37.465" y2="69.85" width="0" layer="20"/>
<wire x1="0" y1="11.43" x2="11.43" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="58.42" x2="11.43" y2="69.85" width="0" layer="20" curve="90"/>
<wire x1="58.42" y1="0" x2="69.85" y2="11.43" width="0" layer="20" curve="-90"/>
<wire x1="58.42" y1="69.85" x2="69.85" y2="58.42" width="0" layer="20" curve="90"/>
<text>RRG</text>
<text>Power Distribution
Rev 1
Max 36V, 130A</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>BATT</text>
<text>5V</text>
</plain>
<libraries>
<library name="custom">
<packages>
<package name="XT60">
</package>
<package name="3921">
</package>
<package name="TSSOP8">
</package>
<package name="DF13-6P">
</package>
<package name="MOLEX_705530002">
</package>
<package name="MATED_POWERPOLE_25A_CONNECTOR">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="custom" package="XT60" value="XT60"/>
<element name="U$3" library="custom" package="3921" value="SHUNT_RES3921"/>
<element name="U1" library="custom" package="TSSOP8" value="LT6100">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402-CAP" value="220pF">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="1k">
<attribute name="NAME"/>
</element>
<element name="J2" library="custom" package="DF13-6P" value="DF13-6P"/>
<element name="C1" library="SparkFun-Capacitors" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U$5" library="custom" package="MOLEX_705530002" value="MOLEX_705530002"/>
<element name="U$2" library="custom" package="MATED_POWERPOLE_25A_CONNECTOR" value="MATED_POWERPOLE_25A_CONNECTOR"/>
<element name="U$4" library="custom" package="MATED_POWERPOLE_25A_CONNECTOR" value="MATED_POWERPOLE_25A_CONNECTOR"/>
<element name="U$6" library="custom" package="MATED_POWERPOLE_25A_CONNECTOR" value="MATED_POWERPOLE_25A_CONNECTOR"/>
<element name="U$7" library="custom" package="MATED_POWERPOLE_25A_CONNECTOR" value="MATED_POWERPOLE_25A_CONNECTOR"/>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="PANASONIC_D" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="V_BATT">
<contactref element="U$3" pad="P$2"/>
<contactref element="U1" pad="1"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="J2" pad="6"/>
<contactref element="J2" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="-"/>
</signal>
<signal name="RAW_BATT">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$5" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="CURRENT_SENSE">
<contactref element="U1" pad="5"/>
<contactref element="J2" pad="3"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VOLT_SENSE">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
