<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="41.265" x2="-1.27" y2="5.715" width="0" layer="20"/>
<wire x1="-1.27" y1="5.715" x2="0.635" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="3.81" x2="28.245" y2="3.81" width="0" layer="20"/>
<wire x1="28.245" y1="3.81" x2="30.15" y2="5.715" width="0" layer="20" curve="90"/>
<wire x1="30.15" y1="5.715" x2="30.15" y2="41.265" width="0" layer="20"/>
<wire x1="30.15" y1="41.265" x2="28.245" y2="43.17" width="0" layer="20" curve="90"/>
<wire x1="28.245" y1="43.17" x2="0.635" y2="43.17" width="0" layer="20"/>
<wire x1="0.635" y1="43.17" x2="-1.27" y2="41.265" width="0" layer="20" curve="90"/>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>DOOR</text>
<text>DATA</text>
<text>RJ-45 Pinout:
3 - VCC (3v3 or 5v)
4 - OneWire Data
5 - GND
6 - Door</text>
<text>DATA</text>
<text>VCC</text>
<text>GND</text>
<text>RJ-45 Breakout Board
v1.1
@thorrak says hi</text>
<text>GND</text>
<text>DOOR</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>DATA</text>
<text>DATA</text>
<text>DOOR</text>
<text>GND</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Donnie">
<packages>
<package name="RJ45-NS-XDIM">
<description>&lt;b&gt;RJ45 Low Profile&lt;/b&gt; No Shield&lt;p&gt;
For all RJ45 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Donnie" package="RJ45-NS-XDIM" value="RJ45-8X">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RJ45-8X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6101"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="U$2" library="holes" package="3,0" value=""/>
<element name="U$3" library="holes" package="3,0" value=""/>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ONEWIRE">
<contactref element="J1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="DOOR">
<contactref element="JP4" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="X1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
