<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="59.416" y2="0" width="0" layer="20"/>
<wire x1="59.416" y1="0" x2="59.416" y2="17.45" width="0" layer="20"/>
<wire x1="59.416" y1="17.45" x2="0" y2="17.45" width="0" layer="20"/>
<wire x1="0" y1="17.45" x2="0" y2="0" width="0" layer="20"/>
<text>Board by NI2O
07/2014</text>
<text>FT8*7 Speech Compressor</text>
</plain>
<libraries>
<library name="analog-devices">
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO8">
<description>&lt;b&gt;8-Lead Small Outline IC&lt;/b&gt; (SO-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="analog-devices" package="SO8" value="SSM2165-1S">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RADIO" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="MIC" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="C1" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="EIA3216" value="22uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="100n"/>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1n"/>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="100n"/>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="100n"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="22k"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="620"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="180K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="RADIO" pad="2"/>
<contactref element="RADIO" pad="5"/>
<contactref element="MIC" pad="2"/>
<contactref element="MIC" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="C"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="RADIO" pad="6"/>
<contactref element="MIC" pad="6"/>
<contactref element="C1" pad="A"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="7"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="SCAN">
<contactref element="RADIO" pad="1"/>
</signal>
<signal name="PTT">
<contactref element="RADIO" pad="3"/>
<contactref element="MIC" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="MIC" pad="1"/>
</signal>
<signal name="MICIN">
<contactref element="RADIO" pad="4"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="MICOUT">
<contactref element="MIC" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="UP">
<contactref element="RADIO" pad="7"/>
<contactref element="MIC" pad="7"/>
</signal>
<signal name="DOWN">
<contactref element="RADIO" pad="8"/>
<contactref element="MIC" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="A"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="C6" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="C3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
