<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="10.1475" y2="0" width="0" layer="20"/>
<wire x1="10.1475" y1="0" x2="10.1475" y2="20.31" width="0" layer="20"/>
<wire x1="10.1475" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X08" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINY85-20PU">
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1455162"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="7"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="13"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="14"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="12"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
