<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="80.01" y2="0" width="0" layer="20"/>
<wire x1="80.01" y1="0" x2="80.01" y2="80.01" width="0" layer="20"/>
<wire x1="80.01" y1="80.01" x2="0" y2="80.01" width="0" layer="20"/>
<wire x1="0" y1="80.01" x2="0" y2="0" width="0" layer="20"/>
<hole x="11.43" y="68.58" drill="3.2512"/>
<hole x="11.43" y="11.43" drill="3.2512"/>
<hole x="68.58" y="68.58" drill="3.2512"/>
<hole x="68.58" y="11.43" drill="3.2512"/>
</plain>
<libraries>
<library name="cree">
<packages>
<package name="VLMU3100">
</package>
</packages>
</library>
<library name="AP2331">
<packages>
<package name="SOT23-5">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Passives" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED2" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED3" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED4" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED5" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED6" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="IC1" library="AP2331" package="SOT23-5" value="AP3015">
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="1210" value="10µH">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="MBRA140">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="68kΩ">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="DCJACK_2MM_SMT" value="2.1MMJACKSMT"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED8" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED9" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED10" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED11" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED12" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED13" library="cree" package="VLMU3100" value="VLMU3100"/>
<element name="LED14" library="cree" package="VLMU3100" value="VLMU3100"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="LED6" pad="K"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
<contactref element="LED12" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED6" pad="A"/>
<contactref element="LED5" pad="K"/>
</signal>
<signal name="N$4">
<contactref element="LED5" pad="A"/>
<contactref element="LED4" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$7">
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="PWR1"/>
<contactref element="JP1" pad="PWR2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LED12" pad="A"/>
<contactref element="LED11" pad="K"/>
</signal>
<signal name="N$13">
<contactref element="LED11" pad="A"/>
<contactref element="LED10" pad="K"/>
</signal>
<signal name="N$15">
<contactref element="LED9" pad="A"/>
<contactref element="LED8" pad="K"/>
</signal>
<signal name="N$16">
<contactref element="LED8" pad="A"/>
<contactref element="LED7" pad="K"/>
</signal>
<signal name="N$5">
<contactref element="LED9" pad="K"/>
<contactref element="LED13" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="LED3" pad="K"/>
<contactref element="LED14" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="LED13" pad="K"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="LED14" pad="K"/>
<contactref element="LED4" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
