<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="158.75" y2="0" width="0" layer="20"/>
<wire x1="158.75" y1="0" x2="161.29" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="161.29" y1="2.54" x2="161.29" y2="28.575" width="0" layer="20"/>
<wire x1="161.29" y1="28.575" x2="158.75" y2="31.115" width="0" layer="20" curve="90"/>
<wire x1="158.75" y1="31.115" x2="2.54" y2="31.115" width="0" layer="20"/>
<wire x1="2.54" y1="31.115" x2="0" y2="28.575" width="0" layer="20" curve="90"/>
<wire x1="0" y1="28.575" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X8">
</package>
</packages>
</library>
<library name="ECA_LEDs">
<packages>
<package name="SC08-21SRWA">
<description>&lt;h1&gt;SC08-21SRWA&lt;/h1&gt;
&lt;h3&gt;Kingbright - 20.32mm (0.8INCH) SINGLE DIGIT NUMERIC DISPLAY&lt;/h3&gt;
&lt;p&gt;The Super Bright Red source color devices are made with Gallium Aluminum Arsenide Red Light Emitting Diode.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;0.8 inch digit height.&lt;/li&gt;
&lt;li&gt;Low current operation.&lt;/li&gt;
&lt;li&gt;Excellent character appearance.&lt;/li&gt;
&lt;li&gt;High light output.&lt;/li&gt;
&lt;li&gt;Easy mounting on P.C. boards or sockets.&lt;/li&gt;
&lt;li&gt;Mechanically rugged.&lt;/li&gt;
&lt;li&gt;Standard : gray face, white segment.&lt;/li&gt;
&lt;li&gt;RoHS compliant.&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="PP_Connectors">
<packages>
<package name="MOUNT_HOLE_150MIL">
</package>
</packages>
</library>
<library name="ECA_Aesthetics">
<packages>
<package name="PINDUINO_LOGO">
</package>
<package name="ECA_LOGO_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="ECA_LEDs" package="SC08-21SRWA" value="SC08-21SRWA">
<attribute name="PARTNO" value="SC08-21SRWA"/>
<attribute name="VALUE" value="SC08-21SRWA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MASTER" library="SparkFun-Connectors" package="2X8" value="M08X2">
<attribute name="PARTNO" value="302-S161"/>
<attribute name="NAME"/>
</element>
<element name="H21" library="PP_Connectors" package="MOUNT_HOLE_150MIL" value="MOUNT_HOLE150MIL"/>
<element name="H1" library="PP_Connectors" package="MOUNT_HOLE_150MIL" value="MOUNT_HOLE150MIL"/>
<element name="H2" library="PP_Connectors" package="MOUNT_HOLE_150MIL" value="MOUNT_HOLE150MIL"/>
<element name="H3" library="PP_Connectors" package="MOUNT_HOLE_150MIL" value="MOUNT_HOLE150MIL"/>
<element name="U$1" library="ECA_Aesthetics" package="PINDUINO_LOGO" value=""/>
<element name="U$2" library="ECA_Aesthetics" package="ECA_LOGO_SMALL" value="">
<attribute name="VERSION" value="1.0.3"/>
<attribute name="YEAR" value="2017"/>
<attribute name="PROJECT" value="Player Display"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MASTER" pad="16"/>
</signal>
<signal name="STB_1">
<contactref element="MASTER" pad="9"/>
<contactref element="D1" pad="4"/>
<contactref element="D1" pad="9"/>
<contactref element="D1" pad="12"/>
<contactref element="D1" pad="17"/>
</signal>
<signal name="STB_2">
<contactref element="MASTER" pad="10"/>
<contactref element="D2" pad="4"/>
<contactref element="D2" pad="9"/>
<contactref element="D2" pad="12"/>
<contactref element="D2" pad="17"/>
</signal>
<signal name="STB_3">
<contactref element="MASTER" pad="11"/>
<contactref element="D3" pad="4"/>
<contactref element="D3" pad="9"/>
<contactref element="D3" pad="12"/>
<contactref element="D3" pad="17"/>
</signal>
<signal name="STB_4">
<contactref element="MASTER" pad="12"/>
<contactref element="D4" pad="4"/>
<contactref element="D4" pad="9"/>
<contactref element="D4" pad="12"/>
<contactref element="D4" pad="17"/>
</signal>
<signal name="STB_5">
<contactref element="MASTER" pad="13"/>
<contactref element="D5" pad="4"/>
<contactref element="D5" pad="9"/>
<contactref element="D5" pad="12"/>
<contactref element="D5" pad="17"/>
</signal>
<signal name="STB_6">
<contactref element="MASTER" pad="14"/>
<contactref element="D6" pad="4"/>
<contactref element="D6" pad="9"/>
<contactref element="D6" pad="12"/>
<contactref element="D6" pad="17"/>
</signal>
<signal name="SEG_A">
<contactref element="D1" pad="2"/>
<contactref element="MASTER" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="SEG_B">
<contactref element="D1" pad="15"/>
<contactref element="MASTER" pad="4"/>
<contactref element="D2" pad="15"/>
<contactref element="D3" pad="15"/>
<contactref element="D4" pad="15"/>
<contactref element="D5" pad="15"/>
<contactref element="D6" pad="15"/>
<contactref element="D7" pad="15"/>
</signal>
<signal name="SEG_C">
<contactref element="D1" pad="13"/>
<contactref element="MASTER" pad="6"/>
<contactref element="D2" pad="13"/>
<contactref element="D3" pad="13"/>
<contactref element="D4" pad="13"/>
<contactref element="D5" pad="13"/>
<contactref element="D6" pad="13"/>
<contactref element="D7" pad="13"/>
</signal>
<signal name="SEG_D">
<contactref element="D1" pad="11"/>
<contactref element="MASTER" pad="8"/>
<contactref element="D2" pad="11"/>
<contactref element="D3" pad="11"/>
<contactref element="D4" pad="11"/>
<contactref element="D5" pad="11"/>
<contactref element="D6" pad="11"/>
<contactref element="D7" pad="11"/>
</signal>
<signal name="SEG_E">
<contactref element="D1" pad="5"/>
<contactref element="D1" pad="7"/>
<contactref element="MASTER" pad="1"/>
<contactref element="D2" pad="5"/>
<contactref element="D2" pad="7"/>
<contactref element="D3" pad="5"/>
<contactref element="D3" pad="7"/>
<contactref element="D4" pad="5"/>
<contactref element="D4" pad="7"/>
<contactref element="D5" pad="5"/>
<contactref element="D5" pad="7"/>
<contactref element="D6" pad="5"/>
<contactref element="D6" pad="7"/>
<contactref element="D7" pad="5"/>
<contactref element="D7" pad="7"/>
</signal>
<signal name="SEG_G">
<contactref element="D1" pad="14"/>
<contactref element="MASTER" pad="5"/>
<contactref element="D2" pad="14"/>
<contactref element="D3" pad="14"/>
<contactref element="D4" pad="14"/>
<contactref element="D5" pad="14"/>
<contactref element="D6" pad="14"/>
<contactref element="D7" pad="14"/>
</signal>
<signal name="SEG_DP">
<contactref element="D1" pad="10"/>
<contactref element="MASTER" pad="7"/>
<contactref element="D2" pad="10"/>
<contactref element="D3" pad="10"/>
<contactref element="D4" pad="10"/>
<contactref element="D5" pad="10"/>
<contactref element="D6" pad="10"/>
<contactref element="D7" pad="10"/>
</signal>
<signal name="SEG_F">
<contactref element="D1" pad="3"/>
<contactref element="MASTER" pad="3"/>
<contactref element="D2" pad="3"/>
<contactref element="D3" pad="3"/>
<contactref element="D4" pad="3"/>
<contactref element="D5" pad="3"/>
<contactref element="D6" pad="3"/>
<contactref element="D7" pad="3"/>
</signal>
<signal name="STB_7">
<contactref element="MASTER" pad="15"/>
<contactref element="D7" pad="4"/>
<contactref element="D7" pad="9"/>
<contactref element="D7" pad="12"/>
<contactref element="D7" pad="17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
